Pella® Lifestyle Series Awning
Aluminum EnduraClad® Exterior
Detailed Product Descriptions

Frame 
•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are clear pine.
•	Exterior surfaces are clad with aluminum. 
•	Components are assembled with screws, staples and concealed corner locks.
•	Overall frame depth is 5" (127 mm) for a wall depth of 3-11/16" (94 mm).
•	Optional factory-applied jamb extensions available between 3-13/16" (97) and 9-3/16" (233).
•	Optional factory-installed fold-out installation fins with flexible fin corners.
•	Optional factory-applied EnduraClad® exterior trim.
•	Optional factory-installed Pella Steady Set Installation System.
Sash 
•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are clear pine.
•	Exterior surfaces are clad with aluminum, lap-jointed and sealed. 
•	Corners mortised and tenoned, glued and secured with metal fasteners. 
•	Sash thickness is [1-3/4" (45 mm) dual-pane] [2-3/16" (55mm) triple-pane, (2-1/4" (57 mm) including hinged glass panel)].
Weatherstripping 
•	Dual weatherstripping. 
•	Flexible santoprene material compressed between frame and sash for positive seal on all four sides. 
•	Secondary thermoplastic vulcanizate (TPV) weatherstrip between edge of sash and frame [Dual-Pane: leaf-type on the vertical sides and bottom side, and Santoprene® bulb-type weatherstrip on the top side] [Triple-Pane: leaf-type on all four sides].
Glazing System
•	Quality float glass complying with ASTM C 1036.
•	High altitude glazing available.
•	Silicone-glazed 11/16" [obscure] [clear] dual-seal insulating glass [[annealed] [tempered]] [[Advanced] [SunDefense™] [SunDefense+] [AdvancedComfort] [NaturalSun] [NaturalSun+] Low-E with argon]]. 
-or-
•	Triple-Pane Glazing System:
•	Exterior silicone-glazed 11/16" [obscure] [clear] dual-seal insulating glass, [[annealed] [tempered]] [[Advanced] [SunDefense™] [SunDefense+] [AdvancedComfort] [NaturalSun] [NaturalSun+] Low-E with argon].
•	Interior hinged glass panel set in a [veneered fiberglass composite] [aluminum (advanced comfort)] frame finished to match interior (aluminum frames are veneered for stain finishes), fitted to sash with continuous gasket seal, clear [annealed] [tempered] glass.
•	Airspace between insulating glass and hinge glass panel is 1-1/32".
Exterior
•	Exterior aluminum surfaces are finished with EnduraClad® protective finish, in a multi-step, baked-on finish. 
•	Finish color [Standard [Black] [White] [Brown] [Fossil]] [Feature [Iron Ore] Wolf gray] [Classic White] [Almond] [Portobello] [Putty] [Brick Red] [Hartford Green]].
Interior
•	[Unfinished, ready for site finishing] [factory primed with one coat acrylic latex] [factory prefinished [White] [Linen White] [Bright White] [stain1]].

Hardware 
•	Roto operator assembly
•	Steel worm gear sash operator with hardened gears.
•	Operator base to be zinc die cast with painted finish. 
•	Operator linkage, hinge slide, and hinge arms are stainless steel. 
•	Exposed fasteners are stainless steel. 
•	Hardware will exceed 1,000 hours salt spray exposure per ASTM B 117. 
•	Vent units are available with operator located [Dual-pane glazing: left or right side as viewed from the exterior] [Triple-pane glazing: on the sill]. 
•	Innovative Locking System — A single handle locking system which operates positive-acting arms that reach out and pull the sash into a locked position: one operating lock installed on units with lock-side frame dimension ≤ 41" , two unison operating locks are installed on units with lock-side frame dimension > 41".
•	Vent units lock handles are located one on each jamb. 
•	Standard Integrated fold-away crank and lock handle finish is [baked enamel [Champagne] [White] [Brown] [Matte Black]] [Satin Brass] [Satin Nickel].
Optional Products
Grilles
•	Simulated-Divided-Light [with optional spacer] (Dual-pane glazing)
•	7/8" Grilles permanently bonded to the interior and exterior of glass.
•	Patterns are [Traditional] [Prairie] [Cross] [Top Row] [Custom – Equally Divided].
•	Interior surfaces are [unfinished, ready for site finishing] [factory primed] [pine: factory prefinished [White] [Linen White] [Bright White] [stain1]].
•	Exterior color to match the exterior cladding color.
•	Simulated-Divided-Light with Grilles-Between-the-Glass (Triple-pane glazing)
•	3/4" Grilles permanently bonded to the exterior of glass.
•	Patterns are [Traditional] [Prairie] [Cross] [Top Row] [Custom – Equally Divided].
•	Exterior color to match the exterior cladding color.
•	Insulating glass contains 3/4" contoured aluminum grilles permanently installed between two panes of glass.
•	Interior color is [White] [Ivory] [Tan3] [Brickstone3] [Black] [Putty3] [Brown] [Harvest] [Cordovan].
– or –
•	Grilles-Between-the-Glass2
•	Insulating glass contains 3/4" contoured aluminum grilles permanently installed between two panes of glass.
•	Patterns are [Traditional] [9-Lite Prairie] [Top Row] [Cross] [Custom – Equally Divided].
•	Interior color is [White] [Ivory] [Tan3] [Brickstone3] [Black] [Putty3] [Brown] [Harvest] [Cordovan].
•	Exterior color [matched to the exterior cladding color] [White]4.
Flat Insect Screen
•	InView™ Screens
•	Vinyl-coated 18/18 mesh fiberglass screen cloth complying with the performance requirements of SMA 1201, set in aluminum frame fitted to inside of window, supplied complete with all necessary hardware.
•	Screen frame finish is baked enamel, [Champagne] [White] [Brown] [Black].
Integrated Between-the-Glass Window Fashions (Triple-Pane glazing only)1
•	Slimshade® Blinds
•	15 mm aluminum slat, bottom-up blinds with polyester cord ladder
•	Installed in sash between double glazing and interior hinged glass panel.
•	Operated with cordless operator or motorized with Insynctive® technology. 
– or –
•	Cellular Fabric Shades
•	11/16" width, bottom-up shades with hidden polyester cord, spun bond Polyethylene Terephthalate (PET) cellular fabric.
•	Installed in sash between double glazing and interior hinged glass panel.
•	Operated with cordless operator or motorized with Insynctive® technology. 
Hardware
•	Optional factory applied limited opening hardware available for vent units in stainless steel; nominal 3" opening.
Sensors
•	Optional factory installed integrated security sensors available in vent units.

(1) Contact your local Pella sales representative for current designs and color options.
(2) Available on units glazed with Low-E insulated glass with argon, and obscure insulated glass.
(3) Tan, brickstone and putty Interior GBG colors are available only with matching interior and exterior colors.
(4) Appearance of exterior grille color will vary depending on Low-E coating on glass.