Pella® Lifestyle Series Sliding Patio Door
Aluminum EnduraClad® Exterior
Detailed Product Descriptions

Frame 
•	Head and jambs are aluminum with fiberglass thermal breaks.
•	Low-profile solid fiberglass sill with Black finish.
•	Interior trim is pine edge banded and veneered and finished to match panel interiors.
•	Exterior surfaces are aluminum at the head and jambs.
•	Components are assembled with screws and corner locks.
•	Optional factory-installed fold-out installation fins with flexible fin corners.
•	Fin position will accommodate standard 4-9/16" (116 mm) wall depths.
•	Frame depth is 5-7/8" (149 mm).
•	Optional supplied jamb extensions available between 4-9/16" (116 mm) and 7-3/16" (183 mm) wall depths.
•	Optional factory-applied EnduraClad® exterior trim.
Door Panels 
•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are veneered with clear pine with no visible fastener holes.
•	Exterior surfaces are clad with aluminum.
•	Panel stiles have LVL core and veneered on interior face.
•	Panel rails are constructed with randomly finger-jointed blocks laminated with water-resistant glue and veneered on interior face.
•	Corners are secured with metal fasteners and structural adhesive.
•	Panel thickness is 2-1/16" (52 mm).
•	Vent panels have two adjustable ABEC 5 sealed electroplated steel ball-bearing rollers with organic coating, set on stainless steel track, standard. 
– or –
•	Two adjustable corrosion-resistant stainless steel ball-bearing rollers; out-of-unit option.
Weatherstripping 
•	Flexible polymeric leaf section with overlapped corners and a slip-coating at head and jamb.
•	Dual-durometer extruded polymer with bulb at sill and interlocker.
Glazing System
•	Quality fully-tempered float glass complying with ASTM C 1048.
•	High altitude insulating glass is available.
•	Silicone-glazed, 3/4" double-pane, dual-seal, insulating glass 
•	[Obscure] with air. 
•	[Obscure Low-E with [argon][air]] [Advanced Low-E] [AdvancedComfort Low-E] [SunDefense™ Low-E] [NaturalSun Low-E] with [argon] [air]. 
– or –
•	Triple-Pane Glazing System:
•	Exterior dual-seal insulating glass, silicone-glazed 3/4", [obscure] [[Advanced] [SunDefense™] [SunDefense+] [AdvancedComfort] [NaturalSun] [NaturalSun+] Low-E [with argon]].
•	Interior hinged clear tempered glass panel set in a [veneered (for stain fishes)] aluminum frame, fitted to door panel with continuous gasket seal.
•	Airspace between insulating glass and hinged glass panel is 1-1/32".
Exterior
•	Aluminum clad exteriors shall be finished with EnduraClad® protective finish, in a multi-step, baked-on finish.
•	Color is [Standard] [Feature] [custom]2.
– or –
•	Aluminum clad exteriors shall be finished with EnduraClad Plus protective finish with 70% fluoropolymer resin in a multi-step, baked-on finish.
•	Color is [Standard] [Feature] [custom]2.

Interior
•	[Unfinished, ready for site finishing] [factory primed with one coat acrylic latex] [factory prefinished [paint] [stain] 2].
Hardware 
•	[Standard Exterior handle finish is matched to exterior cladding finish] [Interior and exterior handle finish is [Satin Brass] [Satin Nickel] [[baked enamel [Champagne] [White] [Brown] [Matte Black]]].
•	Keylock with K-keyway cylinder. Finish is [Chrome].
•	Multi-point locking hardware is electroplated steel with stainless steel strikes.
•	Vent Lock, secondary lock or vents panel open 4", positioned [24" from top for ≤ 96" tall doors] [48" from top for > 96" tall doors] finish is [White] [Black] to correspond with interior panel color.
•	Interior and exterior screen handle finish will be [White] [Black] [Brown] [Fossil] [Morning Sky Gray] to complement screen frame color.
Optional Products
Grilles
•	Simulated Divided Light Grilles
•	Interior grilles are 7/8" solid pine. Interior surfaces are [unfinished, ready for site finishing] [factory primed] [factory prefinished [White] [Linen White] [Bright White] [stain2]].
•	Exterior grilles are 7/8" extruded aluminum.
•	Patterns are [Traditional] [Prairie] [Top Row] [Cross].
•	Insulating glass contains non-glare spacer between the panes of glass.
•	Grilles are adhered to both sides of the insulating glass with VHB acrylic adhesive tape and aligned with spacer
– or –
•	Grilles-Between-the-Glass 3
•	Insulating glass contains 3/4" contoured aluminum grilles permanently installed between two panes of glass.
•	Patterns are [Traditional] [Prairie] [Cross] [Top Row]
•	Interior color is Interior color is [Black] [White] [Brown 4] [Fossil] [Harvest] [Cordovan] [Ivory] [Tan 4] [Brickstone] [Putty 4].
•	Exterior color 5 is [standard] [feature] 2.
Screens
•	InView™ screens
•	Vinyl-coated 18/18 mesh fiberglass screen cloth complying with the performance requirements of SMA 1201, set in aluminum frame, supplied complete with all necessary hardware.
•	Insect screen assembly is top-hung on two adjustable nylon rollers installed on exterior side of door panels. 
•	Screen frame exterior is painted to match exterior color.
•	– or –
•	TuffScreen® by Phifer®
•	Vinyl-coated 17/12.5 mesh polyester screen cloth complying with the performance requirements of SMA 1201, set in aluminum frame, supplied complete with all necessary hardware.
•	Insect screen assembly is top-hung on two adjustable nylon rollers installed on exterior side of door panels. 
•	Screen frame exterior is painted to match exterior color.
Integrated Between-the-Glass Window Fashions (Triple-Pane glazing only)2
•	Slimshade® Blinds 
•	15 mm aluminum slat, bottom-up blinds with polyester cord ladder
•	Installed in sash between double glazing and interior hinged glass panel.
– or –
•	Cellular Fabric Shades
•	11/16" width, bottom-up shades with hidden polyester cord, spun bond Polyethylene Terephthalate (PET) cellular fabric.
•	Installed in sash between double glazing and interior hinged glass panel.

(1) Insulating glass with argon is Low-E coated. All other insulating glass is air-filled.
(2) Contact your local Pella sales representative for current color options.
(3) Available in clear or Low-E insulating glass with argon, and obscure insulated glass.
(4) Tan and Putty Interior GBG colors are available in single-tone (Putty/Putty or Tan/Tan) (Putty mono). Other interior colors are also available with Tan or Brown exterior.
(5) Appearance of exterior grille color will vary depending on Low-E coating on glass. 
The TuffScreen and Pfifer trademarks are property of Phifer Incorporated.