Pella Architect Series® Traditional - In-Swing French Door
Aluminum EnduraClad® Exterior
Detailed Product Descriptions

Frame 
•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are clear pine, edge-banded and veneered. Any curved member may have visible finger-jointed surfaces.
•	Exterior surfaces are clad with aluminum at the head and jambs.
•	Components are assembled with screws, staples and concealed corner locks.
•	Frame depth between 5-7/8" (149 mm) to 8-5/8" (219 mm), for wall depth between 4-9/16" (116 mm) to 7-5/16" (186 mm).
•	Optional factory-applied EnduraClad® exterior trim.
•	Solid extruded aluminum sill with [black] [mill] [satin nickel] [bronze] finish. [Oak] [composite black] threshold.
– or –
•	Sill is 1/2" low profile. Material and finish are extruded aluminum with [mill] [Bronze] finish.
Door Panels 
•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage. 
•	Interior exposed surfaces are veneered with clear pine. Any curved member may have visible finger-jointed surfaces.
•	Exterior surfaces are clad with aluminum.
•	Panel hinge stiles and rails are three-ply construction, randomly finger-jointed blocks laminated with water-resistant glue and veneered on both sides.
•	Panel lock stiles are constructed with LVL core with finger-jointed edge bands on both sides and veneered on both faces.
•	Corners are urethane-silicone hybrid-sealed and secured with metal fasteners.
•	Panel thickness is 2-1/16" (52 mm).
Weatherstripping 
•	Dual-durometer extruded polymer along perimeter of door frame. On bottom panels, dual-durometer extruded polymer interior air seal and rigid polymer exterior facing bristle-strip.
Glazing System
•	Quality fully-tempered float glass complying with ASTM C 1048.
•	Custom and high altitude glazing available. 
•	Urethane-glazed 13/16" dual-seal insulating glass [clear] [obscure] [[Advanced Low-E] [SunDefense™ Low-E] [AdvancedComfort Low-E] [NaturalSun Low-E] with argon]] [[bronze] [gray] [green] Advanced Low-E with argon].
– or –
•	Silicone-glazed 1” triple-pane, dual-seal insulating glass [[annealed][tempered]] [[Advanced Low-E] [SunDefense™ Low-E] [NaturalSun Low-E] with [argon] [krypton]].
– or –
•	Impact-Resistant
•	Urethane-glazed 7/8" dual-seal impact-resistant insulating glass1 PVB. Laminated clear exterior light. Tempered interior light is [Advanced Low-E] [clear] [bronze] [gray] [green].
Exterior 
•	Aluminum clad exteriors shall be finished with EnduraClad® protective finish, in a multi-step, baked-on finish.
•	Color is [Standard] [feature] [custom]1.
							– or – 
•	Aluminum clad exteriors shall be finished with EnduraClad Plus protective finish with 70% fluoropolymer resin in a multi-step, baked-on finish. 
•	Color is [Standard] [feature] [custom]1.
Interior 
•	[Unfinished, ready for site finishing] [factory primed with one coat acrylic latex] [factory prefinished [paint] [stain] 1].

Hardware 

Hinges
•	Hinges are adjustable to help with installation.
•	Doors under 7' 0" frame height will have three (3) hinges per panel.
•	Doors over 7' 0" frame height up to and including 8' 0" frame height will have four (4) hinges per panel.
•	Doors over 8' 3" frame height up to and including 9' 0" frame height will have five (5) hinges per panel.
•	Doors over 9' 0" frame height will have six (6) hinges per panel.
Locks
•	Mortised and keyed multi-point locking system, center deadbolt and shoot-bolts at head and sill will engage simultaneously.
•	Doors 8' 0" frame height and below will have one (1) strike at the head, one (1) strike at the sill and one (1) center deadbolt.
•	Doors over 8' 0" frame height up to and including 10' 0" frame height will have one (1) strike at the head, one (1) strike at the sill and three (3) locking points at the stile.
•	Solid brass handles and keylock with K-keyway cylinder.
•	Key cylinder finish is [Brass] [Stainless Steel] [Matte Black].
Finish
•	Hardware finish is (Handle, Hinges and Strike) [baked enamel [White] [Champagne] [Brown] [Matte Black]] [PVD High Performance finish Satin Nickel] [Oil-Rubbed Bronze] [Distressed Bronze] [Distressed Nickel] [Polished Chrome].
Optional Products
Grilles
•	Integral Light Technology® grilles
•	Interior grilles are [5/8”] [7/8"] [1-1/4"] [2"] ogee profile that are solid pine. Interior surfaces are [unfinished, ready for site finishing] [factory primed] [factory prefinished [paint] [stain] 1].
•	Exterior grilles are [5/8” putty glaze profile] [7/8" [putty glaze] [ogee] profile] [1-1/4" [putty glaze] [ogee] profile] [2" ogee profile] that are extruded aluminum.
•	Patterns are [Traditional] [Prairie] [Top Row] [Cross] [New England] [Victorian].
•	Insulating glass contains non-glare spacer between the panes of glass.
•	Grilles are adhered to both sides of the insulating glass with VHB acrylic adhesive tape and aligned with the non-glare spacer.
– or –
•	Grilles-Between-the-Glass2 
•	Insulating glass contains 3/4" contoured aluminum grilles permanently installed between two panes of glass (exterior air-space on triple-pane insulating glass). 
•	Patterns are [Traditional] [Prairie] [Cross] [Top Row]
•	Interior color is [White] [Tan3] [Brown3] [Putty3] [Black] [Ivory] [Harvest] [Cordovan] [Brickstone].
•	Exterior color4 is [Standard1].
Screens
•	Finish matches exterior cladding.
•	Hinged Insect Screens:
•	Compliance:  ASTM D 3656 and the performance requirements of SMA 1201.
•	Screen Cloth:  InView™ Vinyl-coated fiberglass, 18/18 mesh fiberglass screen cloth.
•	Extruded-aluminum frame, hinged to door frame.
•	Complete with necessary hardware.
•	Hardware Color: [White] [Tan] [Brown].
– or –
•	Exterior Sliding Insect Screens:
•	Compliance:  ASTM D 3656 and the performance requirements of SMA 1201.
•	Screen Cloth:  InView™ Vinyl-coated fiberglass, 18/18 mesh fiberglass screen cloth.
•	Extruded-aluminum frame, top hung on 2 adjustable nylon rollers.
•	Complete with necessary hardware.
•	Hardware Color: [White] [Tan] [Brown].

(1) Contact your local Pella sales representative for current color options.
(2) Available in clear or Low-E insulating glass with argon, and obscure insulated glass.
(3) Tan, Brown or Putty Interior GBG colors are available in single-tone (Brown/Brown, Tan/Tan or Putty/Putty). Other interior colors are also available with Tan or Brown exterior.
(4) Appearance of exterior grille color will vary depending on Low-E coating on glass.