Pella® Fixed Frame Direct Set – Exterior Glazed
Aluminum EnduraClad® Exterior
Detailed Product Descriptions

Frame 
•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage. 
•	Interior exposed surfaces are [clear pine] [mahogany] [douglas fir].
•	Exterior surfaces are clad with aluminum. 
•	Components are assembled with screws, staples, and concealed corner locks.
•	Overall frame depth is 5" (127 mm) for a wall depth of 3-11/16" (94 mm).
•	Optional factory-applied jamb extensions available.
Glazing System1
•	Quality float glass complying with ASTM C 1036.
•	Custom and high altitude glazing available.
•	Butyl-glazed clear single-light with removable aluminum stops.
– or –
•	Urethane-glazed dual-seal insulating glass [[annealed] [tempered]] [[[clear] [[Advanced Low-E] [SunDefense™ Low-E] [AdvancedComfort Low-E] [NaturalSun Low-E] with argon]] [[bronze] [gray] [green] Advanced Low-E with argon] with removable aluminum stops.
Exterior
•	Aluminum clad exteriors shall be finished with EnduraClad® protective finish, in a multi-step, baked-on finish.
•	Color is [standard] [feature] [custom]2.
							– or –
•	Aluminum clad exteriors shall be finished with EnduraClad Plus protective finish with 70% fluoropolymer resin in a multi-step, baked-on finish.
•	Color is [standard] [feature] [custom]2.
Interior
•	[Unfinished, ready for site finishing] [factory primed with one coat acrylic latex] [factory prefinished [paint] [stain] 2].
Optional Products
Grilles
•	Grilles-Between-the-Glass
•	Insulating glass contains 3/4" contoured aluminum grilles permanently installed between two panes of glass.
•	Patterns are [Traditional] [Prairie] [Cross] [Top Row] [Custom – Equally Divided].
•	Interior color is [Black] [White] [Brown3] [Fossil] [Harvest] [Cordovan] [Ivory] [Tan3] [Brickstone] [Putty3].
•	Exterior color4 is [standard] [feature]2.

(1) Insulating glass with argon is Low-E coated (except high altitude). All other insulating glass (including high altitude Low-E) is air-filled.
(2) Contact your local Pella sales representative for current designs and color options.
(3) Tan, Brown and Putty GBG colors are available in single-tone only (Brown/Brown, Tan/Tan or Putty/Putty) (Putty mono), other interior/exterior color restrictions may apply.
(4) Appearance of exterior grille color will vary depending on Low-E coating on glass.