Pella® Fixed Frame Direct Set – Interior Glazed
Aluminum EnduraClad® Exterior
Detailed Product Descriptions

Frame 
•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage. 
•	Interior exposed surfaces are [clear pine] [mahogany] [douglas fir].
•	Exterior surfaces are clad with extruded aluminum. 
•	Components are assembled with screws, staples, and concealed corner locks.
•	Curved glass stops are segmented. 
•	Curved head assembly shall be mitered at end where joined to non- curved frame members, screwed and sealed.
•	Curved head assembly consists of solid wood core blocks bonded to stabilized wood fiber with water-resistant glue. Two sheets are laminated with veneers at interior.
•	Overall frame depth is 5" (127 mm) for a wall depth of 3-11/16" (94 mm).
•	Optional factory-applied jamb extensions available.
•	Optional factory-applied EnduraClad® exterior trim.
Glazing System
•	Quality float glass complying with ASTM C 1036.
•	Custom and high altitude glazing available.
•	Urethane-glazed [13/16"] [1"] dual-seal insulating glass [[annealed] [tempered]] [[clear] [Advanced Low-E] [SunDefense™ Low-E] [AdvancedComfort Low-E] [NaturalSun Low-E] with argon]] [[bronze] [gray] [green] [obscure] Advanced Low-E with argon].
– or –
•	Urethane-glazed [1-1/8"] [1-1/4"] [1-3/8"] triple-seal insulating glass [[annealed] [tempered]] [[Advanced Low-E] [Advanced Low-E] [SunDefense™ Low-E] [SunDefense™ Low-E] [NaturalSun Low-E [NaturalSun Low-E with [argon]].
– or –
•	Impact-Resistant
•	Urethane-glazed 1" dual-seal impact-resistant insulating glass 1 [1" [SGP] [PVB]] [1-1/4" SGP]. [[tempered] [annealed]] Laminated exterior light is [[Advanced Low-E with argon] [SunDefense Low-E] [clear] [bronze] [gray] [green]]. Clear tempered interior light. 
Exterior
•	Extruded aluminum clad exteriors shall be finished with EnduraClad® protective finish, in a multi-step, baked-on finish.
•	Color is [standard] [feature] [custom]2.
– or –
•	Extruded aluminum clad exteriors shall be finished with EnduraClad Plus protective finish with 70% fluoropolymer resin in a multi-step, baked-on finish. 
•	Color is [standard] [feature] [custom]2.
Interior
•	[Unfinished, ready for site finishing] [factory primed with one coat acrylic latex] [factory prefinished [paint] [stain] 2].

Optional Products
Grilles5
•	Integral Light Technology® grilles – Traditional Style Collection
•	Interior grilles are [5/8" putty profile] [7/8" [ogee] [putty] profile] [1-1/4" [ogee] [putty] profile] [2" [ogee] [putty] profile (traditional pattern only)] that are solid [pine] [mahogany] [douglas fir]. Interior surfaces are [unfinished, ready for site finishing] [factory primed] [pine: factory prefinished [paint2] [stain2] to match interior finish]. Curved grilles may have visible finger joints.
•	Exterior grilles are [5/8" putty profile] [7/8" [ogee] [putty] profile] [1-1/4" [ogee] [putty] profile] [2" [ogee] [putty] profile (traditional pattern only)] that are extruded aluminum, color matched to exterior cladding. 
•	Insulating glass contains non-glare spacer between the panes of glass. 
•	Grilles are adhered to both sides of the insulating glass with VHB acrylic adhesive tape and aligned with the non-glare spacer.
•	Grille pattern is [Traditional] [Prairie] [Top Row] [Cross] [Sunburst] [Starburst].
– or –
•	Integral Light Technology® grilles – Contemporary Style Collection (rectangular and angled shapes only)
•	Interior grilles are [5/8"] [7/8"] [1-1/4"] [2"] square profile that are solid [pine] [mahogany] [douglas fir]. Interior surfaces are [unfinished, ready for site finishing] [factory primed] [pine: factory prefinished [paint] [stain] 2 to match interior finish].
•	Exterior grilles are [5/8"] [7/8"] [1-1/4"] [2"] square profile that are extruded aluminum, color matched to exterior cladding. 
•	Insulating glass contains non-glare spacer between the panes of glass. 
•	Grilles are adhered to both sides of the insulating glass with VHB acrylic adhesive tape and aligned with the non-glare spacer.
•	Grille pattern is [Traditional] [Prairie] [Top Row] [Cross].
– or –
•	Simulated-Divided-Light grilles [with optional spacer]
•	Interior grilles are 7/8" regular profile that are solid pine. Curved grilles may have visible finger joints. Interior surfaces are [unfinished, ready for site finishing] [factory prefinished [paint2] [stain2] to match interior finish].
•	Exterior grilles are 7/8" regular profile extruded aluminum, color matched to exterior cladding.
•	Grilles permanently bonded to the interior and exterior of glass with VHB acrylic adhesive tape and are aligned with the optional spacer between the panes of insulating glass.
•	Grille Pattern is [Traditional] [Prairie] [Top Row] [Cross] [Sunburst] [Starburst]
•	Available only on units glazed with Low-E insulated glass with argon.
– or –
•	Grilles-Between-the-Glass3 
•	Insulating glass contains 3/4" contoured aluminum grilles permanently installed between two panes of glass.
•	Interior color is [Black] [White] [Brown4] [Fossil] [Harvest] [Cordovan] [Ivory] [Tan4] [Brickstone] [Putty4]
•	Exterior color6 is [Standard] [Feature]2.
•	Grille pattern is [Traditional] [Prairie] [Cross] [Top Row] [Sunburst].

(1) Insulating glass with argon is Low-E coated (except high altitude). All other insulating glass (including high altitude Low-E) is air-filled.
(2) Contact your local Pella sales representative for current color options.
(3) Available in clear or Low-E insulating glass with argon, and obscure insulated glass.
(4) Tan, Brown and Putty GBG colors are available in single-tone only (Brown/Brown, Tan/Tan or Putty/Putty), other interior/exterior color restrictions may apply.
(5) Certain grille types and patterns may have restrictions depending on unit size and shape, contact your local Pella sales representative for details.
(6) Appearance of exterior grille color will vary depending on Low-E coating on glass.