Pella® Reserve - Traditional Commercial Out-Swing French Door
Wood Exterior
Detailed Product Descriptions

Frame 
•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior and exterior surfaces are [pine] [mahogany]. 
•	Sill is 1/2" low profile. Material and finish are extruded aluminum with [mill] [Bronze] [anodized [Clear] [Light Bronze] [Dark Bronze] [Black] [Custom1]] finish.
•	Overall frame depth is 4-9/16" (116 mm).
•	Jamb extensions available to adapt door to wall thickness between 4-9/16" (116 mm) to 7" (178 mm).
Door Panels 
•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are veneered with [pine] [mahogany]. 
•	Panel stiles and rails are five-ply construction, randomly finger-jointed blocks laminated with water-resistant glue and veneered on both sides.
•	Corners are urethane-silicone hybrid sealed and secured with metal fasteners.
•	Panel thickness is 2-1/16" (52 mm).
Weatherstripping 
•	Dual-durometer extruded polymer along jambs, head and sill.
•	Dual-durometer extruded polymer rainscreen along top and sides of panel.  
•	Bristle rainscreen along bottom of panel.
Glazing System
•	Quality fully-tempered float glass complying with ASTM C 1048.
•	Custom and high altitude glazing available.
•	Urethane-glazed 13/16" dual-seal insulating glass [clear] [obscure] [[Advanced Low-E] [SunDefense™ Low-E] [AdvancedComfort Low-E] [NaturalSun Low-E] with argon]] [[bronze] [gray] [green] Advanced Low-E with argon].
– or –
•	Silicone-glazed 1” triple-pane, dual-seal insulating glass [[annealed] [tempered]] [[Advanced Low-E] [SunDefense™ Low-E] [NaturalSun Low-E] with [argon] [krypton]].
Interior 
•	[Pine [primed with one coat acrylic latex] [Unfinished, ready for site finishing] [prefinished stained1]] [mahogany: Unfinished, ready for site finishing].
Exterior 
•	[Wood composite: primed with one coat acrylic latex] [mahogany: [unfinished, ready for site finishing] [primed with one coat acrylic latex]].
Hardware 
Hinges
•	Ball-bearing hinges 
•	Doors 6' 10" and under frame height will have three (3) ball-bearing hinges.
•	Doors over 6' 10" frame height up to and including 8' 0" frame height will have four (4) ball bearing hinges.
•	Hinge finish [Colonial Bronze (Light Bronze, Dark Bronze, Black anodized sill finishes)] [Satin Nickel (Mill or Clear anodized sill finishes)] to complement the finish of the sill.
– or –
•	Adjustable hinges to assist in installation1.
•	Doors 6' 10" to 7' 0" frame height will have three (3) hinges.
•	Doors over 7' 0" frame height up to and including 8' 0" frame height will have four (4) hinges.
•	Doors over 8' 3" frame height up to and including 9' 0" frame height will have five (5) hinges.
•	Doors over 9' 0" frame height will have six (6) hinges.

Optional Products
Grilles
•	Integral Light Technology® grilles
•	Interior grilles are [5/8”] [7/8"] [1-1/4"] ogee profile that are solid [pine] [mahogany]. Interior surfaces are [unfinished, ready for site finishing] [factory primed] [pine: factory prefinished [paint] [stain] 1 ].
•	Exterior grilles are [5/8”] [7/8"] [1-1/4"] putty glaze profile that are solid [pine] [mahogany]. Exterior surfaces are water repellent, preservative-treated in accordance with WDMA I.S.-4, and are [unfinished, ready for site finishing] [factory primed]. 
•	Patterns are [Traditional] [Prairie] [Top Row] [Cross] [New England] [Victorian].
•	Insulating glass contains non-glare spacer between the panes of glass.
•	Grilles are adhered to both sides of the insulating glass with VHB acrylic adhesive tape and aligned with spacer.
– or –
•	Grilles-Between-the-Glass2 
•	Insulating glass contains 3/4" contoured aluminum grilles permanently installed between two panes of glass (exterior air-space on triple-pane insulating glass). 
•	Patterns are [Traditional] [Prairie] [Cross] [Top Row]
•	Interior color is [Black] [White] [Brown3] [Fossil] [Harvest] [Cordovan] [Ivory] [Tan3] [Brickstone] [Putty3].
•	Exterior color4 is [standard1].
Intermediate Rail and Flat Panel Options
•	6" Intermediate rail is three-ply construction, randomly finger-jointed blocks laminated with water-resistant glue and veneered on both sides.
•	Wood Flat panel exterior is an LVL construction with exposed surfaces that are veneered with [pine] [mahogany]. Exteriors are [pine: primed] [mahogany [primed] [unfinished, ready for site finishing]].  
•	Flat panel is an LVL construction with Interior exposed surfaces are veneered with [pine] [mahogany].
•	Standard placement: 6" Intermediate Rail 38" OC from the bottom of the door sill

(1) Contact your local Pella sales representative for current color options.
(2) Available in clear or Low-E insulating glass with argon, and obscure insulated glass.
(3) Tan, Brown or Putty Interior GBG colors are available in single-tone (Brown/Brown, Tan/Tan or Putty/Putty). Other interior colors are also available with Tan or Brown exterior.
(4) Appearance of exterior grille color will vary depending on Low-E coating on glass.