Pella Corporation	May 2024
102 Main Street
Pella, Iowa 50219
Toll Free	(800) 54-PELLA
Phone		(641) 621-1000
Website	www.pella.com

	Product Guide Specification

Specifier Notes:  This product guide specification is written according to the Construction Specifications Institute (CSI) 3-Part Format, including MasterFormat, SectionFormat, and PageFormat, contained in The Project Resource Manual--CSI Manual of Practice.

The section must be carefully reviewed and edited by the Architect to meet the requirements of the project and local building code.  Coordinate this section with other specification sections and the Drawings.  Delete all “Specifier Notes” when editing this section.

Section numbers are from MasterFormat 2020.	

	SECTION 08 18 16

	FIBERGLASS SLIDING DOORS

Specifier Notes:  This section covers Pella® Impervia® sliding doors.  Frame and panels are manufactured from, a five-layer, pultruded-fiberglass material, reinforced with a Pella-patented interlocking mat.  Consult your local Pella representative for assistance in editing this section for the specific application.	

PART 1	GENERAL

1.1	SECTION INCLUDES

A.	Fiberglass sliding doors.

1.2	RELATED SECTIONS

Specifier Notes:  Edit the following list of related sections as required for the project.  List other sections with work directly related to this section.  Verify section numbers and titles.	

A.	Section 07270 (07 27 00) - Air Barriers:  Water-resistant barrier.

B.	Section 07920 (07 92 00) - Joint Sealants:  Sealants and caulking.

1.3	REFERENCES

Specifier Notes:  List standards referenced in this section, complete with designations and titles.  This article does not require compliance with standards, but is merely a listing of those used.	

A.	American Architectural Manufacturers Association (AAMA):
1.	AAMA 502 - Voluntary Specification for Field Testing of Windows and Sliding Doors.
2.	AAMA 624 - Voluntary Performance Requirements and Test Procedures for Organic Coatings on Fiber Reinforced Thermoset Profiles.

B.	American Society for Testing and Materials (ASTM):
1.	ASTM C 1036 - Flat Glass.
2.	ASTM C 1048 - Heat-Treated Flat Glass--Kind HS, Kind FT Coated and Uncoated Glass.
3.	ASTM D 3656 - Insect Screening and Louver Cloth Woven from Vinyl-Coated Glass Yarns.
4.	ASTM E 283 - Rate of Air Leakage Through Exterior Windows, Curtain Walls and Doors Under Specified Pressure Difference Across the Specimen.
5.	ASTM E 547 - Water Penetration of Exterior Windows, Curtain Walls and Doors by Cyclic Static Air Pressure Differential.
6.	ASTM E 1105 –  Standard Test Method for Field Determination of Water Penetration of Exterior Windows, Doors, Skylights and Curtain Walls by Uniform Static Air Pressure Difference.

C.	Screen Manufacturers Association (SMA):
1.	SMA 1201 - Specifications for Insect Screens for Windows, Sliding Doors and Swinging Doors.

D.	Window and Door Manufacturers Association (WDMA):
1.	ANSI/AAMA/NWWDA 101/I.S.2 - Voluntary Specifications for Aluminum, Vinyl (PVC) and Wood Windows and Glass Doors.

1.4	PERFORMANCE REQUIREMENTS

Specifier Notes:  Performance ratings for Pella Impervia doors vary by product and size.  Current performance information is found in the Pella Impervia Architectural Design Manual at www.pellaadm.com on the Design Data pages of each product section.  Consult your local Pella representative for more information.	

A.	Doors shall meet Rating SGD-LC-PG[ _____ ] specifications in accordance with ANSI/AAMA/NWWDA 101/I.S.2/A440-08.

B.	Door Air Leakage, ASTM E 283:  Door air leakage when tested at 1.57 psf (25 mph) shall be 0.15 cfm/ft2 of frame or less.

Specifier Notes:  Specify static pressure. 	

C.	Door Water Penetration, ASTM E 547:  No water penetration through door when tested under static pressure of [5.25 psf (45 mph)] [6.75 psf (51 mph)] [7.5 psf (55 mph)] after 4 cycles of 5 minutes each, with water being applied at a rate of 5 gallons per hour per square foot.

1.5	SUBMITTALS

A.	Submit in accordance with Division 1 requirements.

B.	Product Data:  Submit manufacturer's product data, including installation instructions.

Specifier Notes:  Delete the following sentence if shop drawings are not required.	

C.	Shop Drawings:  Submit manufacturer's shop drawings, indicating dimensions, construction, component connections and locations, anchorage methods and locations, hardware locations, and installation details.

Specifier Notes:  Delete the following sentence if samples are not required.	

D.	Samples:  Submit full-size or partial full-size sample of door illustrating glazing system, quality of construction, and color of finish.

1.6	QUALITY ASSURANCE

Specifier Notes:  Edit the following paragraph as required for inclusion of field testing.	

A.	Mockup:
1.	Provide sample installation for field testing door performance requirements and to determine acceptability of door installation methods.
2.	Approved mockup shall represent minimum quality required for the Work.

Specifier Notes:  Edit the following sentence as required for inclusion of the mockup.	

3.	Approved mockup shall [not] remain in place within the Work.

1.7	DELIVERY, STORAGE, AND HANDLING

A.	Delivery:  Deliver materials to site undamaged in manufacturer's or sales branch's original, unopened containers and packaging, with labels clearly identifying manufacturer and product name.  Include installation instructions.

B.	Storage:
1.	Store materials in accordance with manufacturer's instructions.
2.	Store materials off ground and under cover.
3.	Protect materials from weather, direct sunlight, and construction activities.

C.	Handling:  Protect materials and finish during handling and installation to prevent damage.

PART 2	PRODUCTS

2.1	MANUFACTURER

A.	Pella Corporation, 102 Main Street, Pella, Iowa 50219.  Toll Free (800) 54-PELLA.  Phone (641) 621-1000.  Website www.pella.com.

2.2	FIBERGLASS SLIDING DOORS

A.	Sliding Doors:  Pella Impervia.

Specifier Notes:  Specify frame assembly type.  All doors over 96” in height and 4 panel doors require site assembly.	

1.	[Factory-assembled door with panel installed in frame] [Knock down site assembled frame and panel].
2.	Frame and Panel Material: 5-layer, pultruded-fiberglass material, reinforced with interlocking mat.

Specifier Notes:  Specify frame type.  Block frames can be used in new block walls or in replacement door applications.  New construction frames have a factory applied vinyl fin on jambs and head.	

B.	Frame:
1.	Type: [Block frame] [New construction frame].
2.	Interior and Exterior Frame: Pultruded, fiberglass composite [with foam inserts].
3.	Overall Frame Depth:  5 inches.
4.	Overall Sill height 1-1/8 inches.
5.	Nominal Wall Thickness of Fiberglass Members:  0.070 inch to 0.120 inch.
6.	Frame Corners:
a.	Mitered.
b.	Joined and bonded with moisture curing, hot-melt silicone adhesive, glass filled polypropylene corner lock, and mechanically fastened.

Specifier Notes:  Include the following sentence when specifying block frames. Installation clips are not included in block frame install and should be specified separately.	

7.	Head and Jambs:  Factory-drilled, counter-bored, installation screw holes.
8.	Sill:  Black painted finish. 

C.	Door Panels:
1.	Interior and Exterior Panel: Pultruded, fiberglass composite [with foam inserts].
2.	Vent Panel:  Removable for cleaning exterior glass.
3.	Panel Corners:
a.	Mitered.
b.	Bonded and injected with moisture curing, hot-melt silicone adhesive.

D.	Glazing:
1.	Float Glass:  ASTM C 1036, Quality 1.
a.	Tempered Glass:  ASTM C 1048.
Specifier Notes:  Specify dual-pane or triple-pane insulating glass.
2.	Dual-Pane Insulating Glass: Moisture curing hot-melt glazed, 1-inch thick, [High-altitude] insulating glass.
Specifier Notes:  Specify type of dual-pane insulating glass.  Delete glass types and gas fill not required.  Consult your local Pella representative for more information. SunDefenseTM Low-E coated insulating glass is a Trademark of Pella Corporation.
a.	Clear
b.	Advanced Low-E coated, [with argon].
c.	“SunDefense” Low-E coated, [with argon].
d.	“NaturalSun” Low-E coated, [with argon].
e.	Bronze Advanced Low-E coated, [with argon].
f.	Gray Advanced Low-E coated, [with argon].
g.	Bronze Advanced Low-E coated, [with argon].
h.	Obscure:  Low-E coated, [with argon].

3.	Triple-Pane Insulating Glass: Moisture curing hot-melt glazed, 1 inch thick, [High-altitude] insulating glass.
Specifier Notes:  Specify type of triple-pane insulating glass.  Delete glass types and gas fill not required. Consult your local Pella representative for more information.
a.	Advanced Low-E coated, [with argon].
b.	“NaturalSun” Low-E coated, [with argon].
c.	“SunDefense” Low-E coated, [with argon].

4.	Impact Resistant Insulating Glass: Silicone-glazed 1" dual-seal impact-resistant insulating glass PVB. tempered exterior light is [[multi-layer Low-E coated] [clear]]. Laminated [[clear] [bronze][ interior light.

E.	Weather Stripping:
1.	Dual weather strip at all locations.

a.	All vent panel polymer seals are slip coated.
b.	Weather strip overlaps in corners.
c.	Vent panel lock Jamb has a bristle rain screen on exterior with an interior polymer leaf air seal.
d.	Vent panel head has a polymer leaf seal on exterior and interior.
e.	Vent panel sill has a bristle rain screen on exterior with a polymer interior bulb air seal.
f.	Interlocker has a bristle rain screen on exterior with an interior polymer bulb air seal.
g.	Fixed panel has a polymer leaf rain screen on exterior with a foam compression interior air seal.

2.3	OPTIONS

Specifier Notes:  The following paragraphs specify optional products.  Specify required options.  Consult your local Pella representative for more information.	

A.	Grilles:
1.	Insulating Glass:  Contain 3/4-inch, contoured, aluminum grilles between the glass.
2.	Finish:  Factory-finished.  Match door frame.

Specifier Notes:  Blinds are only available on select sizes. Specify clear glass if blinds are selected. Consult your local Pella representative for more information.	
B.	Blinds:  Blinds-between-the-glass.
2.	Aluminum blinds sealed between Clear Low-E dual-pane insulating glass.
3.	Operation:  Cordless tilt, raise, and lower.
4.	Color:  [White] [Slate Gray] [Espresso].

Specifier Notes:  If insect screens are not specified, delete ASTM D 3656 and SMA 1201 from Article 1.3 References in this section.	
C.	Sliding Insect Screens:  Standard.
1.	Compliance:  ASTM D 3656 and SMA 1201.
2.	Screen Cloth:  Vinyl-coated fiberglass, 18/18 mesh.

Specifier Notes:  Specify color.	

3.	Extruded-Aluminum Frame: [White] [Brown] [Black] [Tan] [Morning Sky Gray].
4.	Rollers:  Top hung on 2 adjustable nylon rollers, exterior side of door panels.
5.	Strike:  Frame-mounted strike.
6.	Hardware:  Complete with necessary hardware.
7.	Interior and Exterior Handle and Latch Finish:  Match extruded-aluminum frame finish.

Specifier Notes:  Optional sill spacer to aid in compliance to ADA standards. Consult local code authorities for approval of use.	
D.	Sill Option:
	1.	Extruded-Aluminum Accessibility Sill Filler. 

2.4	HARDWARE

A.	Handles:
1.	Interior Handle and Thumb Lock:

Specifier Notes:  Specify finish.	

 a.	Finish: [Powder-coat paint [White] [Brown] [Matte Black] [Tan] [Morning Sky Gray] [Satin nickel].

Specifier Notes:  Key lock is optional.  Sliding doors have a plug in the exterior handle as standard.  The finish of the plug matches the door handle finish.	

2.	Exterior Handle is powder-coat painted to match exterior.

Specifier Notes: Specify finish of key cylinder.	

	a.	Key Cylinder Finish: [Matte Black] [Chrome].

B.	Locking System:
1.	Multiple-Point Lock Hardware: Electroplated steel with stainless steel adjustable strike.
2.	Secure Vent Lock holds the door open approximately 3" for ventilation, available in two height locations, color matched to interior.

C.	Vent Panel Rollers:

1.	Two adjustable, permanently sealed, electroplated steel with organic coating, ball-bearing rollers, set on stainless steel track.

2.5	TOLERANCES

A.	Doors shall accommodate the following opening tolerances:
1.	Horizontal Dimensions Between High and Low Points:  Plus 1/4-inch, minus 0 inch.
2.	Width Dimensions:  Plus 1/4-inch, minus 0 inch.
3.	Building Columns or Masonry Openings:  Plus or minus 1/4-inch from plumb.

2.6	FINISH

A.	Exterior and Interior Finish:  Factory-applied powder-coat paint, comply with AAMA 624.

Specifier Notes:  Specify one of the following two sentences. 	

1.	Color: [White] [Tan] [Brown] [Morning Sky Gray] [Black].
2.	Dual-color: [Brown] [Black] exterior with White interior.

2.7	INSTALLATION ACCESSORIES

A.	Flashing/Sealant Tape:  Pella SmartFlash.
1.	Aluminum-foil-backed butyl window and door flashing tape.
2.	Maximum Total Thickness:  0.013 inch.
3.	UV resistant.
4.	Verify sealant compatibility with sealant manufacturer.

B.	Interior Insulating-Foam Sealant:  Low-expansion, low-pressure polyurethane insulating 
	window and door foam sealant.

C.	Exterior Perimeter Sealant: “Pella Window and Door Installation Sealant” or equivalent high quality, multi-purpose sealant as specified in the joints sealant section.

Specifier Notes:  Specify one of the following installation accessories to attach the door to the opening when specifying block frames.	

D.	Block Frame Installation Accessories: [Vinyl installation fin] [Vinyl installation fin with head drip flashing] [Offset vinyl installation fin] [Installation clips] [Installation screws for frame screw applications].

PART 3	EXECUTION

3.1	EXAMINATION

A.	Examine areas to receive doors.  Notify Architect of conditions that would adversely affect installation or subsequent use.  Do not proceed with installation until unsatisfactory conditions are corrected.

3.2	INSTALLATION

A.	Install doors in accordance with manufacturer's instructions.

B.	Install doors to be weather-tight and freely operating.

C.	Maintain alignment with adjacent work.

D.	Secure assembly to framed openings, plumb and square, without distortion.

Specifier Notes:  The following paragraph applies to doors installed using installation fins only.  If the doors are not being installed with installation fins, delete this paragraph.	

E.	Integrate door system installation with exterior water-resistant barrier using flashing/sealant tape. Apply and integrate flashing/sealant tape with water-resistant barrier using watershed principles in accordance with door manufacturer's instructions.

F.	Place interior seal around door perimeter to maintain continuity of building thermal and air barrier using [insulating-foam sealant] [backer-rod and sealant].

G.	Seal door to exterior wall cladding with sealant and related backing materials at perimeter of assembly.

H.	Leave doors closed and locked.

3.3	FIELD QUALITY CONTROL

Specifier Notes:  Field testing is optional.  Delete Field Quality Control if field testing is not required.  If Field Quality Control is deleted, delete AAMA 502 from Article 1.3 References in this section.	

A.	Field Testing:  Field water testing shall be conducted in accordance with ASTM E1105 Test Procedure B. The test pressure shall be based on the maximum positive components and cladding design pressure. Utilizing the AAMA 502 field test reduction, the water test pressure is 10% of the maximum positive design pressure.

3.4	CLEANING

A.	Clean door frames and glass in accordance with Division 1 requirements.

B.	Do not use harsh cleaning materials or methods that would damage finish or glass.

C.	Remove labels and visible markings.

3.5	PROTECTION

A.	Protect installed doors to ensure that, except for normal weathering, doors will be without damage or deterioration at time of substantial completion.

END OF SECTION