Pella® Reserve - In-Swing French Casement 
Aluminum EnduraClad® Exterior
Detailed Product Descriptions

Frame 
•	Select woods, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are [pine] [mahogany] [douglas fir] (standard rectangular units only). Any curved member may have visible finger-jointed surfaces.
•	Exterior surfaces are clad with aluminum. 
•	Overall frame depth is 5" (127 mm) for a wall depth of 3-11/16" (94 mm).
•	Optional factory-applied jamb extensions available between 4-9/16" (116 mm) and 7-3/16" (183 mm) wall depths.
Sash 
•	Select woods, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are clear [pine] [mahogany] [douglas fir] (standard rectangular units only). Any curved member may have visible finger-jointed surfaces.
•	Exterior surfaces are clad with aluminum and sealed. 
•	Corners mortised and tenoned, glued and secured with metal fasteners. 
•	Sash thickness is 2-3/4" (69 17/20 mm) for [11/16"] or [1"] glazings.
•	Exterior sash profile is [ogee] [putty glaze], interior sash profile is ogee. 
Weatherstripping 
•	Dual weather stripping. 
•	A foam filled close cell sheathed weather-strip on the full frame perimeter is compressed between frame and sash for positive seal on all four sides.
•	Secondary leaf-type weather strip between edge of sash and frame.
Glazing System1
•	Quality float glass complying with ASTM C 1036.
•	Silicone-glazed 11/16" dual-seal insulating glass [[annealed] [tempered]] [[clear] [Advanced Low-E coated with argon]] [SunDefense™ Low-E with Argon] [AdvancedComfort Low-E] [NaturalSun Low-E] [[bronze] [gray] [green] air-filled Advanced Low-E coated]].
•	Custom and high altitude glazing available for 11/16" glazing only.  
– or –
•	Silicone-glazed triple-pane 1-1/16” dual-seal insulating glass [[annealed] [tempered]] [[Advanced Low-E with argon] [Advanced Low-E with krypton] [SunDefense™ Low-E with argon] [SunDefense™ Low-E with krypton] [NaturalSun Low-E with krypton] [Obscure [standard] [fern]].
Exterior
•	Exterior aluminum surfaces are finished with EnduraClad® multi-stage finish system.
•	Color is [Standard] [Feature] [custom]2. 
– or –
•	Exterior aluminum surfaces are finished with EnduraClad Plus 70% fluoropolymer-based multi-stage finish system. 
•	Color is [Standard] [Feature] [custom]2.
Interior
•	[Unfinished, ready for site finishing] [Factory-primed with one coat acrylic latex] [Pine: [Factory prefinished [paint] [stain] 2].
Hardware 
•	Multi-point lock system—A dual handle locking system engages multiple locking points around the sash.
•	Finish of handle is [baked enamel, [Champagne] [White] [Brown]] [Satin Brass] [Satin Nickel] [Oil-Rubbed Bronze]. All vent units are available with active/passive- or passive/active hinging.

Optional Products
Grilles
•	Integral Light Technology® grilles
•	Interior grilles are [5/8”] [7/8"] [1-1/4"] [2"] ogee profile that are solid [Pine] [Mahogany] [Douglas Fir]. Interior surfaces are [unfinished, ready for site finishing] [factory primed] [pine: factory prefinished [paint] [stain] 2].
•	Exterior grilles are [5/8” putty profile] [7/8" [putty] [ogee] profile] [1-1/4" [putty] [ogee] profile] [2" ogee profile] that are extruded aluminum.
•	Patterns are [Traditional] [Prairie] [Top Row] [Cross] [New England] [Victorian] [Simulated French].
•	Insulating glass contains non-glare spacer between the panes of glass.
•	Bars are adhered to both sides of the insulating glass with VHB acrylic adhesive tape and aligned with the non-glare spacer.
– or –
•	Grilles-Between-the-Glass 3
•	Insulating glass contains 3/4” contoured aluminum grilles permanently installed between two panes of glass (exterior air-space on triple-pane insulating glass).
•	Patterns are [Traditional] [Prairie] [Cross] [Top Row] [Custom – Equally Divided].
•	Interior color is [Black] [White] [Brown4] [Fossil] [Harvest] [Cordovan] [Ivory] [Tan4] [Brickstone] [Putty4].
•	Exterior color5 is [Standard] [Feature]2.
Screen
•	InView™ Screens
•	[Full-Size] black vinyl-coated 18/18 mesh fiberglass screen cloth complying with SMA 1201, set in aluminum frame fitted to outside of window, supplied complete with all necessary hardware.
•	Screen frame finish is baked enamel, color to match window cladding.

(1) Insulating glass with argon is Low-E coated (except high altitude). All other insulating glass (including high altitude Low-E) is air-filled.
(2) Contact your local Pella sales representative for current color options.
(3) Available in clear or Low-E and obscure insulating glass.
(4) Tan, Brown and Putty Interior GBG colors are available in single-tone (Brown/Brown, Tan/Tan or Putty/Putty). Other interior colors are also available with Tan or Brown exterior.
(5) Appearance of exterior grille color will vary depending on Low-E coating on glass.