Vinyl Windows and Doors Manufactured by Pella Corporation
Single-Hung – East and West Regions
Detailed Product Description

Frame
•	Overall frame depth: 2-11/16" [new construction frame with integral nailing fin [and J-channel (East region only)]] [3-1/4" replacement frame with optional sill adapter and head expander] [replacement frame [with integral flush flange (Florida region only)].
•	Frame members are extruded, [high impact-resistant (2-11/16” frame, East Only)], rigid uPVC [with optional foam insulation1].
•	Frame members are mitered and heat-fused to provide a fully welded corner assembly.
Sash
•	Sash members are extruded, rigid uPVC [with optional foam insulation1].
•	Sash members are mitered and heat-fused to provide a fully welded corner assembly.
•	Integral extruded sash lift at checkrail.
Weatherstripping
•	Fin-type pile around the perimeter of the vent sash.
Glazing System2
•	Quality float glass complying with ASTM C1036, Quality.
•	Exterior face glazed 3/4" sealed insulating glass.
•	[Clear] [[Advanced] [SunDefense™] [SunDefense+] [NaturalSun] [NaturalSun+] [Advanced Comfort (West region only)] [bronze, Advanced (East Region only)] Low-E [with Argon]]; [Clear] [NaturalSun Low-E] [Standard obscure [Fern (West region only)] [Rain] [High Altitude [with argon] (West region only)]. [tempered].
Interior / Exterior
•	All window frame members have an integral color extruded throughout the profiles.
•	All exposed PVC surfaces are smooth, glossy and uniform in appearance.
•	East Region Finish color [White] [Almond] [Fossil] (all frame types); West Region Finish color [White (all frame types)] [[Almond] [Fossil] (Nail Fin frame only)].
Hardware
•	Constant force balances connected to sash with stainless steel spring and concealed within the frame.
•	Lower sash is fully operable for ventilation.
•	All fasteners are corrosion-resistant material compatible with uPVC.
•	Lock is factory installed zinc die cast self-aligning cam-action lock located on the checkrail.
•	2-11/16” Units ≥ 29-1/2" wide have two locks.
•	Integral extruded sash lift.
•	Tilt latches are factory installed and located on the checkrail (East region Only).
•	Hardware is factory pre-finished to match unit.
Optional Products	
•	Primed wood jamb extensions available on 2-1/8" wall depth frame-for [4-9/16"] and [6-9/16"] frame depth. 
Grilles
•	Grilles-Between-the-Glass
•	Insulating glass contains [3/4" contoured (East or West)] [5/8" flat (West)] aluminum grilles permanently installed between two panes of glass.
•	Grilles match color of interior and exterior frame.
Hardware
•	Drywall Pass Through option is available on fin frame, single units of frame size greater or equal to 29.5'' x 59.5''.
•	Dry-wall Pass Through option is available on fin frame two wide composites with individual units of frame size greater or equal to 29.5'' x 59.5'' and less than or equal to 35.5'' x 71.5''.
•	Optional limited opening hardware available for field installation on vent units in [White] [Almond] extruded vinyl to match the interior of the unit; nominal 3-3/4" opening. 
•	Optional window opening control device available for field installation. Device allows window to open less than 4” with normal operation, with a release mechanism that allows the sash to open completely. Complies with ASTM F2090-10.
Screens
•	Half-size with black vinyl coated 18/14 mesh fiberglass screen cloth complying with FS L-S125B, ASTM D 3656 and SMA 1201.
•	Set in aluminum frame and fitted to outside of window.
•	Supplied complete with all necessary hardware.

(1) Foam insulation inserts are not available with clear glazing.
(2) SunDefense+ and NaturalSun+ are only available with argon fill, and are not available for obscure glass.