Vinyl Windows and Doors Manufactured by Pella Corporation
Sliding Patio Door – East and West Regions
Detailed Product Description

Frame
•	Overall frame depth 4-1/2" [new construction frame with continuous integral fin] [replacement frame with double-wall flush flange (West region only)].
•	Frame members are mitered and heat fused to provide a fully welded corner assembly.
•	Interior and exterior frame surfaces extruded, ridged uPVC.
Door Panel
•	Door panel consists of extruded, ridged uPVC.  
•	Panel members are mitered and heat fused to provide a fully welded corner assembly.  
•	Vent panels have two adjustable rollers, set on stainless steel track cap.
Weather stripping
•	Fin-type pile around perimeter of vent panel.
Glazing System
•	Quality float glass complying with ASTM C1036.
•	Exterior faced glazed 3/4" Tempered [[clear] [Advanced] [SunDefense™] [SunDefense+] [NaturalSun] [NaturalSun+] [bronze, Advanced (East Region only)] Low-E coated [with Argon]]; [Clear] [NaturalSun Low-E] [standard obscure1 [fern (West region only)] [rain (West region only)]] [high altitude [with argon] (West region only)].
or
•	Exterior face glazed 1” tempered Low-E sealed insulating glass with Blinds-Between-the-Glass.
Interior / Exterior
•	All panel frame members have an integral color extruded throughout the profiles.
•	All exposed uPVC surfaces are smooth and uniform in appearance.
•	East Region Finish color [White] [Almond] [Fossil] (all frame types); West Region Finish color [White (all frame types)] [[Almond] [Fossil] (Nail Fin frame only)].
Hardware
•	Interior handle and thumblock; finish is [White] [Almond] [Fossil] [Satin Nickel] [Oil-Rubbed Bronze].
•	Exterior handle and finish is painted [White] [Almond] [Fossil] to match exterior.
•	Vent panel is fully operable for ventilation.
•	All fasteners are a corrosion-resistant material compatible with uPVC.
•	Single-point lock.
•	Door rollers are adjustable, permanently-sealed, electroplated steel with organic coated ball-bearing rollers.
Optional Products	
Grilles
•	Grilles-Between-the-Glass (East Region)
•	3/4" contour aluminum Grilles-Between-Glass.
•	Grille bars are factory pre-finished [White] [Almond] [Fossil].
•	Grilles-Between-the-Glass (West Region)
•	[5/8" flat] [3/4" contour] aluminum Grilles-Between-Glass.
•	Grille bars are factory pre-finished [White] [Almond] [Fossil].
Blinds
•	Blinds-Between-the-Glass
•	White aluminum blinds sealed between dual pane 1” insulating glass.
•	Cordless raise and lower operation.
Hardware
•	Keylock with K-keyway cylinder. Finish is [Chrome].
Screens
•	[Standard coil frame screen] [heavy duty frame screen] full-size with black vinyl coated 18/14 mesh fiberglass screen cloth
complying with ASTM D 3656 and SMA 1201 set in an aluminum frame fitted to door exterior.
•	Supplied with four adjustable rollers, latch and latch handle.

(1) Obscure glass not available with Bronze Advanced, SunDefense+ or NaturalSun+ Low-E IG.