Pella® Architect Series® – Traditional Awning and Large Awning
Aluminum EnduraClad® Exterior
Detailed Product Description

•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are [clear pine] [mahogany] [douglas fir]] [Impact-Resistant: [clear pine] [mahogany]].
•	Exterior surfaces are clad with aluminum.
•	Components are assembled with screws, staples and concealed corner locks.
•	Overall frame depth is 5" (127mm) for a wall depth of 3-11/16" (94mm).
•	Optional factory-applied jamb extensions available between 3-13/16" (97mm) and 9-3/16" (233mm).
•	Optional factory-installed fold-out installation fins with flexible fin corners.
•	Optional factory-applied EnduraClad® exterior trim.
Sash
•	Select softwood, immersion treated with Pella’s EnduraGuard wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage. 
•	Corners are mortised and tenoned, glued and secured with metal fasteners.
•	Interior exposed surfaces are: [clear pine] [mahogany] [douglas fir]] [Impact-Resistant: [clear pine] [mahogany]].
•	Exterior surfaces are clad with extruded aluminum butt-jointed at all corners of the sash with through-stile construction and sealed. 
•	Sash thickness is [1-13/16" (46mm) for 11/16"] [2-1/8" (54mm) for 1"] glazing.
•	Exterior sash profile is ogee, interior sash profile is ogee.
Weatherstripping
•	Dual weatherstripping.
•	Flexible santoprene material compressed between frame and sash for positive seal on all four sides.
•	Secondary thermoplastic vulcanizate (TPV) leaf-type weatherstrip between edge of sash and frame on the vertical sides and bottom, and Santoprene® bulb-type weatherstrip on the top.
Glazing System1
•	Quality float glass complying with ASTM C 1036.
•	Silicone-glazed dual-pane 11/16" dual-seal insulating glass [[annealed] [tempered]], [[clear] [[Advanced Low-E] [SunDefense™ Low-E] [NaturalSun Low-E] [AdvancedComfort Low-E] with argon]] [[bronze] [gray] [green] Advanced Low-E [with Argon]] [obscure] [Reflective Bronze] [Reflective Gray]. 
-or- 
•	Silicone-glazed dual-pane 1" dual-seal tempered spandrel glass [Lava Bronze Amber] [Black] [Ford Blue] [Symmetry Bronze] [Symmetry Gray] [Symmetry Green]. 
-or- 
•	Silicone-glazed dual-pane 11/16" dual-seal [[annealed] [tempered]] non-impact laminated glass [[clear] [[Advanced Low-E] [SunDefense Low-E] with Argon]] [[bronze] [gray] [green] Advanced Low-E [with argon]]. 
– or –
•	Silicone-glazed 1” triple-pane, dual-seal insulating glass [[annealed][tempered]] [[Advanced Low-E] [SunDefense™ Low-E] [NaturalSun Low-E] with [argon]]
– or –
•	Impact-Resistant
•	Silicone-glazed 1" dual-seal impact-resistant insulating glass1 SGP. [[tempered] [annealed]] exterior light is [[Advanced Low-E] [SunDefense] [clear] [bronze] [gray] [green]]. Laminated clear interior light.
– or –
•	Silicone-glazed 11/16" dual-seal impact-resistant insulating glass1 [PVB]. [[tempered] [annealed]] exterior light is [[Advanced Low-E] [SunDefense] [clear]]. Laminated [clear] interior light, or [[tempered] [annealed]] exterior light is [multi-layer Low-E]. Laminated [[bronze] [gray] [green]] interior light.
Exterior
•	Aluminum clad exteriors shall be finished with EnduraClad® protective finish, in a multi-step, baked-on finish.
•	Color is [Standard] [Feature] [custom]2.
– or –
•	Aluminum clad exteriors shall be finished with EnduraClad Plus protective finish with 70% fluoropolymer resin in a multi-step, baked-on finish.
•	Color is [Standard] [Feature] [custom]2.
Interior
•	[Unfinished, ready for site finishing] [factory primed with one coat acrylic latex] [factory prefinished [paint] [stain] 2].

Hardware
•	Roto operator assembly
•	Steel worm gear sash operator with hardened gears.
•	Operator base is zinc die cast with painted finish.
•	Operator linkage is stainless steel.
•	Exposed fasteners are stainless steel.
•	Hardware will exceed 1,000 hours salt spray exposure per ASTM B 117. 
•	Hinge slide and hinge arms are [Awning: Stainless steel] [Large Awning: wash hinge] [Impact-Resistant: wash hinge].
•	All vent units are available with operator located on the [Awning: left or right side as viewed from the exterior] [Large Awning or Impact-Resistant: bottom center of the unit].
•	SureLock® System—A single handle locking system operates positive-acting arms that reach out and pull the sash into a locked position: [Awning: one operating lock installed on units with frame widths 29" and less, two unison operating locks installed on units with frame widths over 29"] [Large Awning: one operating lock installed on units with frame heights 41" and less, two unison operating locks installed on units with frame height over 41"]. 
•	Style of hardware is [Standard integrated fold-away crank and standard lock handle with [baked enamel [Champagne] [White] [Brown] [Matte Black]] [Satin brass] [Satin nickel] [Oil-rubbed bronze] hardware finish]
[Antiek fold-away crank and Antiek lock handle with [baked enamel [Champagne] [White] [Brown] [Matte Black]] [Satin Brass] [Satin Nickel] [Oil-rubbed Bronze] [Distressed Bronze] [Distressed Nickel] hardware finish].
Optional Products
Grilles
•	Integral Light Technology® grilles
•	Interior grilles are [7/8"] [1-1/4"] [2"] ogee profile that are solid [Pine] [mahogany] [douglas fir]. Interior surfaces are [unfinished, ready for site finishing] [factory primed] [pine: factory prefinished [paint] [stain] 2].
•	Exterior grilles are [7/8"] [1-1/4"] [2"] ogee profile that are extruded aluminum.
•	Patterns are [Traditional] [Prairie] [Top Row] [Cross] [New England] [Victorian] [Diamond].
•	Insulating glass contains non-glare spacer between the panes of glass.
•	Grilles are adhered to both sides of the insulating glass with VHB acrylic adhesive tape and aligned with non-glare spacer.
– or –
•	Grilles-Between-the-Glass3
•	Insulating glass contains 3/4” contoured aluminum grilles permanently installed between two panes of glass (exterior air-space on triple-pane insulating glass).
•	Patterns are [Traditional] [Prairie] [Cross] [Top Row] [Custom – Equally Divided].
•	Interior color is [Black] [White] [Brown4] [Fossil] [Harvest] [Cordovan] [Ivory] [Tan4] [Brickstone] [Putty4].
•	Exterior color5 is [Standard2].
Screens
•	InView™ screens
•	Vinyl-coated 18/18 mesh fiberglass screen cloth complying with the performance requirements of SMA 1201, set in aluminum frame fitted to inside of window, supplied complete with all necessary hardware.
•	Screen frame finish is [baked enamel [Champagne] [White] [Brown] [Black]] [Wrapped in wood veneer, factory prefinished stain to match interior finish].
Hardware
•	Optional factory applied limited opening hardware available for vent units in stainless steel; nominal 3" opening.
Sensors
•	Optional factory installed integrated security sensors available in vent units.

(1) Low-E coated insulating glass is argon-filled (except high altitude). All other insulating glass (including high altitude Low-E) is air-filled.
(2) Contact your local Pella sales representative for current designs and color options.
(3) Available in clear or Low-E insulating glass only.
(4) Tan, Brown or Putty Interior GBG colors are available in single-tone (Brown/Brown, Tan/Tan or Putty/Putty). Other interior colors are also available with tan or brown exterior.
(5) Appearance of exterior grille color will vary depending on Low-E coating on glass.