Pella® Reserve – Traditional Double-Hung Windows
Wood Exterior
Detailed Product Description

Frame 
•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are [clear pine] [mahogany] (standard rectangular windows only). Any curved member may have visible finger-jointed surfaces.
•	Exterior surfaces are [pine] [mahogany]. 
•	Overall frame depth is 4-3/8" (111mm) for a wall depth of 4-3/16" (106mm).
•	Vinyl Jamb liner includes wood / clad inserts.
•	Optional factory applied jamb extensions available between 4-5/16" (110mm) and 9-3/16" (233mm).
Sash 
•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are [clear pine] [mahogany (standard rectangular windows only)]. Any curved member may have visible finger-jointed surfaces.
•	Exterior surfaces are [pine] [mahogany].
•	Sash exterior profile is putty glaze, interior profile is ogee.
•	Corners [mortised and tenoned on rectangular units] [mitered on arch head units], glued and secured with metal fasteners. 
•	Sash thickness is 1-7/8" (47mm).
•	[Double-Hung: Upper sash has surface-mounted wash locks] [Single-Hung: Fixed upper sash has surface-mounted wash locks] [Arch Head units have no wash locks].
•	Lower sash has concealed wash locks in lower check rail.
•	Sashes tilt in for easy cleaning.
•	Simulated-Hung units have non-operable upper and lower sashes.
Weatherstripping 
•	Water-stop santoprene-wrapped foam at head and sill. 
•	Thermoplastic elastomer bulb with slip-coating set into lower sash for tight contact at check rail. 
•	Kerf mounted bristle weatherstrip at sill.
•	Vinyl-wrapped foam inserted into jamb liner to seal against sides of sash.
Glazing System
•	Quality float glass complying with ASTM C 1036.
•	Custom and high altitude glazing available.  
•	Silicone-glazed 11/16" dual-seal insulating glass [[annealed] [tempered]] [[clear] [[Advanced] [SunDefense™] [SunDefense+] [AdvancedComfort] [NaturalSun] [NaturalSun+] Low-E [with argon]] [[bronze] [gray] [green] Advanced Low-E with argon].
Exterior
•	[Pine: factory primed with one coat acrylic latex] [Mahogany: [factory primed with one coat acrylic latex] [Unfinished, ready for site finishing]]
Interior 
•	[Unfinished, ready for site finishing] [factory primed with one coat acrylic latex] [pine: factory prefinished [paint] [stain] 1].
Hardware 
•	Galvanized block-and-tackle balances are connected to self-locking balance shoes which are connected to the sashes using zinc die cast terminals and concealed within the frame.
•	Sash lock is [standard (cam-action)] [historic spoon-style] [air-conditioner lock] [simulated lock (Single-piece lock ties upper and lower sash together. When removed, lower sash becomes operable)]. Two sash locks on units with frame width 37" and greater.
•	Optional sash lift furnished for field installation. Two lifts on units with frame width 37" and greater.
•	Hardware finish is [baked enamel [Champagne] [White] [Brown] [Matte Black]] [satin brass] [satin nickel] [oil-rubbed bronze] [distressed bronze] [distressed nickel]. 

Optional Products
Grilles
•	Integral Light Technology® grilles
•	Interior grilles are solid [5/8”] [7/8"] [1-1/4"] ogee profile that are solid [pine] [mahogany]. Interior surfaces are [unfinished, ready for site finishing] [factory primed] [pine: factory prefinished [paint] [stain] 1].
•	Exterior grilles are solid [5/8”] [7/8"] [1-1/4"] putty glaze profile that are [pine] [mahogany]. Exterior surfaces are water repellent, preservative-treated in accordance with WDMA I.S.-4, and are [unfinished, ready for site finishing] [factory primed].
•	Patterns are [Traditional] [Prairie] [Top Row] [New England] [Victorian].
•	Insulating glass contains non-glare spacer between the panes of glass.
•	Grilles are adhered to both sides of the insulating glass with VHB acrylic adhesive tape and aligned with the non-glare spacer.
– or –
•	Grilles-Between-the-Glass2
•	Insulating glass contains 3/4" contoured aluminum grilles permanently installed between two panes of glass.
•	Patterns are [Traditional] [9-Lite Prairie] [Cross] [Top Row]
•	Interior color is [Black] [White] [Brown3] [Fossil] [Harvest] [Cordovan] [Ivory] [Tan3] [Brickstone] [Putty3].
•	Exterior color5 is [standard1].
Screens
•	InView™ screens
•	[Half-Size] [Full-Size4] black vinyl-coated 18/18 mesh fiberglass screen cloth complying with the performance requirements of SMA 1201, set in a [standard roll-form] [premium extruded] aluminum frame aluminum frame fitted to outside of window, supplied complete with all necessary hardware.
•	Full screen spreader bar placed on units > 37" width or > 65" height.
•	Insect screen frame finish is baked enamel.
Hardware
•	Optional factory applied limited opening device available for vent units in stainless steel; nominal 3-3/4" opening. Limiting device concealed from view.
•	Optional factory applied window opening control device.  Device allows window to open less than 4” with normal operation, with a release mechanism that allows the sash to open completely.  Complies with ASTM F2090-10.
Sensors
•	Optional factory installed integrated security sensors available in vent units.

(1) Contact your local Pella sales representative for current designs and color options.
(2) Available in clear or Low-E insulating glass only.
(3) Tan, Brown and Putty Interior GBG colors are available in single-tone (Brown/Brown, Tan/Tan or Putty/Putty). Other interior colors are also available with Tan or Brown exterior.
(4) Full screens are available on units ≤ 96" height.
(5) Appearance of exterior grille color will vary depending on Low-E coating on glass.