Pella® Reserve™ – Double-Hung Windows with Impact-Resistant Glass
Aluminum EnduraClad® Exterior
Detailed Product Description

Frame 
•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are [clear pine] [mahogany].
•	Exterior surfaces are clad with aluminum. 
•	Components are assembled with screws, staples and concealed corner locks.
•	Vinyl Jamb liner includes wood/clad inserts.
•	Overall frame depth is 5-7/8" (149 mm) for a wall depth of 4-9/16" (116 mm).
•	Optional factory applied jamb extensions available from 4-9/16" (116 mm) and 7-3/16" (183 mm) wall depths.
•	Optional factory installed fold-out installation fins with flexible fin corners.
•	Optional factory-applied EnduraClad® exterior trim.
Sash 
•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are [clear pine] [mahogany (not available if sash weight > 200 lbs.)].
•	Exterior surfaces are clad with extruded aluminum and sealed. 
•	Corners mortised and tenoned, glued and secured with metal fasteners. 
•	Sash thickness is 2-1/4" (57 mm).
•	Exterior sash profile is [ogee] [putty glaze], interior profile is ogee.
•	Double-hung upper sash (if sash weight ≤ 92 lbs.) has surface-mounted wash locks for tilt-in cleaning.
•	Double-hung and single-hung lower sash (if sash weight ≤ 92 lbs.) has concealed wash locks in lower check rail for tilt-in cleaning.
Weatherstripping 
•	Santoprene-wrapped foam at head and sill.
•	Full length glass filled polypropylene interlocker with integrated slip-coated thermoplastic elastomer leaf.
•	Secondary nylon bristle rainstrip on lower sash at sill.
•	Vinyl-wrapped foam with secondary nylon bristle rainstrip inserted into jamb liner to seal against sides of sash.
Glazing System
•	Quality float glass complying with ASTM C 1036.
•	Impact-Resistant
•	Silicone-glazed 13/16" dual-seal impact-resistant insulating glass2 PVB. [[tempered] [annealed]] exterior light is [[Advanced Low-E with argon] [clear]]. Laminated [clear] interior light, or [[tempered] [annealed]] exterior light is [[Advanced Low-E] [SunDefense] with argon] [clear]]. Laminated [[bronze] [gray] [green]] interior light.

Exterior 
•	Aluminum-clad exteriors shall be coated with EnduraClad® protective finish, in a multi-step, baked-on finish.
•	Color is [standard] [custom]1.
– or –
•	Aluminum-clad exteriors shall be coated with EnduraClad Plus protective finish with 70% fluoropolymer resin in a multi-step, baked-on finish. 
•	Color is [standard] [custom]1.
Interior 
•	[Unfinished, ready for site finishing] [factory primed with one coat acrylic latex] [factory prefinished [paint] [stain] 1].

Hardware 
•	Galvanized block-and-tackle balances are attached to self-locking balance shoes connected to the sashes using zinc die cast terminals concealed within the frame.
-or-
•	Class 5 hybrid balance attached to [locking] [non-locking] balance shoes connected to the sashes using zinc die cast terminals and concealed within the frame.
-or-
•	Galvanized block-and-tackle balances combined with a Class 5 hybrid balance attached to non-locking balance shoes connected to the sashes using zinc die cast terminals and concealed within the frame.
•	All balances comply with AAMA 902 specification
•	Lock hardware is [standard lock (cam-action)] [spoon-style lock] [air-conditioner lock] [simulated lock (Single-piece lock ties upper and lower sash together. When removed, lower sash becomes operable)]. Two sash locks on all unit widths.
•	Optional sash lift furnished for field installation. Two lifts on unit make width 37" and greater.
•	Hardware Finish is [baked enamel [Champagne] [White] [Brown] [Matte Black]] [Satin Brass] [Satin Nickel] [Oil-Rubbed Bronze] [Distressed Bronze] [Distressed Nickel].
Optional Products
Sash
•	Exterior sash lugs
•	Optional factory applied accessory. Exterior finish is [Standard1] [Custom1].
Grilles
•	Integral Light Technology® grilles
•	Interior grilles are [5/8”] [7/8"] [1-1/4"] [2"] ogee profile that are solid [pine] [mahogany]. Interior surfaces are [unfinished, ready for site finishing] [factory primed] [pine: factory prefinished [paint] [stain] 1].
•	Exterior grilles are [5/8” putty profile] [7/8" [putty glaze] [ogee] profile] [1-1/4" [putty glaze] [ogee] profile] [2" ogee profile] that are extruded aluminum.
•	Patterns are [Traditional] [Prairie] [Top Row] [New England] [Victorian].
•	Insulating glass contains non-glare spacer between the panes of glass.
•	Grilles are adhered to both sides of the insulating glass with VHB acrylic adhesive tape and aligned with the non-glare spacer.
– or –
•	Grilles-Between-the-Glass2 	
•	Insulating glass contains 3/4” contoured aluminum grilles permanently installed between two panes of glass (exterior air-space on triple-pane insulating glass)
•	Patterns are [Traditional] [Prairie] [Cross] [Top Row]
•	Interior color is [White] [Tan3] [Brown3] [Putty3] [Black] [Ivory] [Sand Dune] [Harvest] [Cordovan] [Brickstone].
•	Exterior color4 is [standard1].
Screens
•	InView™ Screens
•	[Full-screen (not available on units > 120” tall)] [half-screen] black Vinyl-coated 18/18 mesh fiberglass screen cloth complying with with the performance requirements of SMA 1201, set in a [extruded (optional on units < 84" height, standard on units >84")] [standard] aluminum frame fitted to outside of window, supplied complete with all necessary hardware.
•	Full screen spreader bar placed on units > 37” width or > 65” height.
•	Screen frame finish is baked enamel, color to match window cladding.
Hardware
•	Optional factory applied limited opening device available for venting units; nominal 3-3/4" opening. Limiting device concealed from view.
•	Optional window opening control device available for field installation. Device allows window to open less than 4” with normal operation, with a release mechanism that allows the sash to open completely. Complies with ASTM F2090-10.
•	Optional [head, sill, stool locks].

(1) Contact your local Pella sales representative for current designs and color options.
(2) Low-E coated insulating glass is argon-filled (except high altitude). All other insulating glass (including high altitude Low-E) is air-filled.
(3) Tan, Brown and Putty Interior GBG colors are available in single-tone (Brown/Brown, Tan/Tan or Putty/Putty). Other interior colors are also available with Tan or Brown exterior.
(4) Appearance of exterior grille color will vary depending on Low-E coating on glass.
(5) Vivid View screen is not available when frame height is > 84" or when both frame width and frame height are > 48".