Pella® Reserve™ - Sliding French Door with Impact-Resistant Glass
Aluminum EnduraClad® Exterior
Detailed Product Description

Frame 
•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are [pine] [mahogany] edge banded and veneered.
•	Exterior surfaces are clad with aluminum at the head and jambs.
•	Components are assembled with screws, staples and concealed corner locks.
•	Solid extruded aluminum sill with Brown EnduraClad® protective finish. [mahogany threshold for mahogany door] [[oak] [composite black] threshold for [pine] door].
•	Optional factory-installed fold-out installation fins with flexible fin corners.
•	Fin position will accommodate standard 4-9/16" (116 mm) wall depths.
•	Frame depth is 5-7/8" (149 mm).
•	Optional factory-applied jamb extensions available between 4-9/16" (116 mm) and 7-3/16" (183 mm) wall depths.
•	Optional factory-applied EnduraClad® exterior trim.
Door Panels
•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are veneered with [pine] [mahogany].
•	Exterior surfaces are clad with aluminum.
•	Panel stiles have LVL core with finger-jointed edge bands on both sides and veneered on both faces.
•	Panel rails are three-ply construction, randomly finger-jointed blocks laminated with water-resistant glue and veneered on both sides.
•	Corners are secured with metal fasteners and structural adhesive.
•	Panel thickness is 2-1/16" (52 mm).
•	Panel exterior profile is [ogee] [putty glaze], interior profile is ogee.
•	Vent panels have two adjustable ABEC 5 sealed electroplated steel ball-bearing rollers with organic coating, set on stainless steel track, standard.
– or –
•	Two adjustable corrosion-resistant stainless steel ball-bearing rollers; out of-unit option.
Weatherstripping
•	Dual-durometer extruded polymer with bulb at head, jamb and threshold. Corners are welded along perimeter of door panels.
Glazing System1
•	Quality fully-tempered float glass complying with ASTM C 1048.
•	Silicone-glazed, [11/16"] [7/8"] double-pane, dual-seal, impact-resistant, laminated, insulating glass
•	PVB Laminated clear exterior light, tempered interior light.
•	Clear with air.
•	[Bronze] [Gray] [Green] with air.
•	[Advanced Low-E] [SunDefense™ Low-E] with argon.
Exterior
•	Aluminum clad exteriors shall be finished with EnduraClad® protective finish, in a multi-step, baked-on finish.
•	Color is [Standard] [custom]2.
– or –
•	Aluminum clad exteriors shall be finished with EnduraClad Plus protective finish with 70% fluoropolymer resin in a multi-step, baked-on finish.
•	Color is [Standard] [custom] 2.
Interior
•	[Unfinished, ready for site finishing] [factory primed with one coat acrylic latex] [factory prefinished [paint] [stain] 2].

Hardware
•	Interior handle and thumb lock finish is [Satin Brass] [Satin Nickel] [Oil-Rubbed Bronze] [Polished Nickel] [Polished Chrome] [Distressed Bronze] [Distressed Nickel] [baked enamel [Champagne] [White] [Brown] [Matte Black]].
•	Exterior handle finish is baked enamel, color to match door cladding.
•	Keylock with K-keyway cylinder.
•	Multiple point lock hardware is electroplated steel with stainless steel strikes.
•	The foot bolt has a Black finish.
Optional Products
Grilles
•	Integral Light Technology®
•	Interior grilles are [5/8”] [7/8"] [1-1/4"] [2"] ogee profile that are solid [Pine] [mahogany]. Interior surfaces are [unfinished, ready for site finishing] [factory primed] [pine: factory prefinished [paint] [stain] 2].
•	Exterior grilles are [5/8” putty profile] [7/8" [putty] [ogee] profile] [1-1/4" [putty] [ogee] profile] [2" ogee profile] that are extruded aluminum, finished to match door cladding.
•	Patterns are [Traditional] [Prairie] [Top Row] [Cross] [New England] [Victorian].
•	Insulating glass contains non-glare spacer between the panes of glass.
•	Grilles are adhered to both sides of the insulating glass with VHB acrylic adhesive tape and aligned with the non-glare spacer
– or –
•	Grilles-Between-the-Glass3
•	Insulating glass contains 3/4" contoured aluminum grilles permanently installed between two panes of glass.
•	Patterns are [Traditional] [Prairie] [Cross] [Top Row]
•	Interior color is [White] [Tan4] [Brown4] [Putty4] [Black] [Ivory] [Sand Dune] [Harvest] [Cordovan] [Brickstone].
•	Exterior color5 is [standard2].
Screens
•	InView™ screens
•	Vinyl-coated 18/18 mesh fiberglass screen cloth complying with with the performance requirements of SMA 1201, set in aluminum frame fitted to inside of door, supplied complete with all necessary hardware.
•	Screen assembly is top-hung on two adjustable nylon rollers installed on room side of door panels.
•	Screen frame exterior is painted to match exterior color.
•	Screen frame interior is [pine] [mahogany] veneer wrapped over extruded aluminum [Unfinished] [prefinished to match door6]. 
– or –
•	Rolscreen® Retractable Screen
•	Self-storing, rolling, black vinyl-coated 18/16 mesh fiberglass screen cloth complying with ASTM D 3656 and SMA 1201 mounted to fixed panel and covered by veneered aluminum.
•	Cover finish is [factory prefinished paint] [[pine] [mahogany] veneer wrapped over extruded aluminum with factory prefinished stain2.
•	Available on two- and three-panel sliding patio doors.

(1) Insulating glass with argon is Low-E coated. All other insulating glass is air-filled.
(2) Contact your local Pella sales representative for current color options.
(3) Available in clear or Low-E insulating glass only.
(4) Tan, Brown and Putty Interior GBG colors are available in single-tone (Putty/Putty, Brown/Brown or Tan/Tan) (Putty mono). Other interior colors are also available with Tan or Brown exterior.
(5) Appearance of exterior grille color will vary depending on Low-E coating on glass. 
(6) Prefinished White interior screen frame is only available with White exterior finish.