Pella® Reserve – Traditional Out-Swing French Door
Aluminum EnduraClad® Exterior
Detailed Product Description

Frame 
•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are [clear pine] [mahogany] [douglas fir], edge-banded and veneered on straight members. Curved members may have finger-jointed surfaces.
•	Exterior surfaces are clad with aluminum at the head and jambs.
•	Components are assembled with screws, staples and concealed corner locks.
•	Frame depth is 5-7/8" (149mm) for a wall depth of 4-9/16" (116mm).
•	Jamb extensions available to adapt door to wall thickness between 4-9/16" (116mm) to 7" (178mm).
•	Optional factory-applied EnduraClad® exterior trim.
•	Solid extruded aluminum sill with [Mill] [Nickel] [Bronze] [Black] [anodized to match anodized cladding] finish. [Mahogany threshold for mahogany door] [[oak] [composite black] threshold for [pine] [douglas fir] door].
– or –
•	Sill is 1/2" low profile. Material and finish is extruded aluminum with [mill] [bronze] [anodized to match anodized cladding] finish.
Door Panels 
•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are veneered with [clear pine] [mahogany] [douglas fir] on straight members. Curved members may have finger-jointed surfaces.
•	Exterior surfaces are clad with extruded aluminum.
•	Panel stiles and rails are three-ply construction, randomly finger-jointed blocks laminated with water-resistant glue and veneered on both sides.
•	Units over 8' height have panel stiles constructed with LVL core with finger-jointed edge bands on both sides and veneered on both faces.
•	Corners are urethane-silicone hybrid sealed and secured with metal fasteners.
•	Panel thickness is 2-1/16" (52mm).
•	Panel exterior profile is [ogee] [putty glaze], interior profile is ogee.
Weatherstripping 
•	Dual-durometer extruded polymer along jambs, head and sill.
•	Dual-durometer extruded polymer rainscreen along top and sides of panel.
•	Bristle rainscreen along bottom of panel.
Glazing System1
•	Quality fully-tempered float glass complying with ASTM C 1048.
•	Custom and high altitude glazing available. 
•	Silicone-glazed, 13/16" double-pane, dual-seal, insulating glass 
•	[Clear] [Obscure] [Reflective Bronze] with air. 
•	[Obscure Low-E with [argon][air]] [Advanced] [AdvancedComfort] [SunDefense™] [SunDefense+] [NaturalSun] [NaturalSun+] Low-E [with argon]]. 
•	[Bronze] [Gray] [Green] Advanced Low-E [with argon].
 - or –
•	Silicone-glazed, 13/16” double-pane, dual-seal, laminated, insulating glass
•	Clear with air.
•	[Advanced] [SunDefense™] Low-E with argon.
•	[Bronze] [Gray] [Green] Advanced Low-E with argon.
– or –
•	Silicone-glazed, 1” triple-pane, dual-seal, insulating glass
•	[Obscure Low-E [with argon]] [Advanced] [SunDefense™] [NaturalSun] Low-E [with argon].
– or –
•	Silicone-glazed, 7/8” double-pane, dual-seal, impact-resistant, laminated, insulating glass
•	Clear with air.
•	[Bronze] [Gray] [Green] with air.
•	[Advanced] [SunDefense™] Low-E with argon.

Exterior 
•	Aluminum clad exteriors shall be finished with EnduraClad® protective finish, in a multi-step, baked-on finish.
•	Color is [Standard] [custom]1.
– or –
•	Aluminum clad exteriors shall be finished with EnduraClad Plus protective finish with 70% fluoropolymer resin in a multi-step, baked-on finish. 
•	Color is [Standard] [custom]1.
Interior 
•	[Unfinished, ready for site finishing] [factory primed with one coat acrylic latex] [factory prefinished [paint] [stain] 1].
Hardware 
Hinges
•	Adjustable hinges standard to assist in installation.
•	Doors 6' 10" to 7' 0" frame height will have three (3) hinges.
•	Doors over 7' 0" frame height up to and including 8' 0" frame height will have four (4) hinges.
•	Doors over 8' 3" frame height up to and including 9' 0" frame height will have five (5) hinges.
•	Doors over 9' 0" frame height will have six (6) hinges.
•	Hinge color to match exterior cladding.
Locks
•	Mortised and keyed multi-point locking system, center deadbolt and shoot-bolts at head and sill will engage simultaneously.
•	Doors 8' 0" frame height and below will have one (1) strike at the head, one (1) strike at the sill and one (1) center deadbolt.
•	Doors over 8' 0" frame height up to and including 10' 0" frame height will have one (1) strike at the head, one (1) strike at the sill and three (3) locking points at the stile.
•	Solid brass handles and keylock with K-keyway cylinder.
•	Key cylinder finish is [Brass] [Stainless Steel] [Matte Black].
Finish
•	Hardware finish is (Handle, Hinges and Strike) [baked enamel [White] [Champagne] [Brown] [Matte Black]] [PVD High Performance finish [Satin Brass] [Satin Nickel]] [Oil-Rubbed Bronze] [Distressed Bronze] [Distressed Nickel] [Polished Nickel] [Polished Chrome].
Optional Products
Grilles
•	Integral Light Technology® Grilles
•	Interior grilles are [5/8"] [7/8"] [1-1/4"] [2"] ogee profile that are solid [pine] [mahogany] [douglas fir]. Interior surfaces are [unfinished, ready for site finishing] [factory primed] [pine: factory prefinished [paint] [stain]1].
•	Exterior grilles are [5/8" putty glaze profile] [7/8" [putty glaze] [ogee] profile]] [1-1/4" putty glaze] [ogee] profile] [2" ogee profile] that are extruded aluminum.
•	Patterns are [Traditional] [Prairie] [Top Row] [Cross] [New England] [Victorian].
•	Insulating glass contains non-glare spacer between the panes of glass.
•	Grilles are adhered to both sides of the insulating glass with VHB acrylic adhesive tape and aligned with spacer.
– or –
•	Grilles-Between-the-Glass2
•	Insulating glass contains 3/4" contoured aluminum grilles permanently installed between two panes of glass (exterior air-space on triple-pane insulating glass). 
•	Patterns are [Traditional] [Prairie] [Cross] [Top Row]
•	Interior color is [Black] [White] [Brown3] [Fossil] [Harvest] [Cordovan] [Ivory] [Tan3] [Brickstone] [Putty3].
•	Exterior color4 is [Standard1].
Sensors
•	Optional factory installed integrated security sensors available in vent units.

(1) Contact your local Pella sales representative for current color options.
(2) Available in clear or Low-E insulating glass only.
(3) Tan, Brown or Putty Interior GBG colors are available in single-tone (Brown/Brown, Tan/Tan or Putty/Putty). Other interior colors are also available with Tan or Brown exterior.
(4) Appearance of exterior grille color will vary depending on Low-E coating on glass.