Pella® Reserve - Contemporary Push Out Casement
Aluminum EnduraClad® Exterior
Detailed Product Descriptions

Frame 
•	Select woods, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are [pine] [mahogany] [douglas fir].
•	Exterior surfaces are clad with aluminum. 
•	Overall frame depth is 5" (127 mm) for a wall depth of 3-11/16" (94 mm).
•	Optional factory-applied jamb extensions available between 4-9/16" (116 mm) and 7-3/16" (183 mm) wall depths.
•	Optional factory-installed fold-out installation fins with flexible fin corners.
•	Optional factory-applied EnduraClad® exterior trim.
Sash 
•	Select woods, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are clear [pine] [mahogany] [douglas fir].
•	Exterior surfaces are clad with extruded aluminum butt-jointed at all corners of the sash with through-stile construction and sealed.
•	Corners mortised and tenoned, glued and secured with metal fasteners. 
•	Sash thickness is [1-13/16" (46 mm) for 11/16"] [2-1/8" (54 mm) for 1"] glazing.
•	Sash exterior profile is square, interior profile is square. 
Weatherstripping 
•	Dual weather stripping. 
•	Flexible santoprene material compressed between frame and sash for positive seal on all four sides. 
•	Secondary thermoplastic vulcanizate (TPV) leaf-type weatherstrip between edge of sash and frame on the vertical sides and bottom side, and Santoprene® bulb-type weatherstrip on the top side.
Glazing System1
•	Quality float glass complying with ASTM C 1036.
•	Silicone-glazed dual-pane 11/16" dual-seal insulating glass [[annealed] [tempered]], [[clear] [[Advanced Low-] [SunDefense™ Low-E] [NaturalSun Low-E] [AdvancedComfort Low-E] with argon]] [[bronze] [gray] [green] Advanced Low-E [with Argon]] [obscure] [Reflective Bronze] [Reflective Gray].
– or –
•	Silicone-glazed dual-pane 1" dual-seal tempered spandrel glass [Lava Bronze Amber] [Black] [Ford Blue] [Symmetry Bronze] [Symmetry Gray] [Symmetry Green].
  – or –
•	Silicone-glazed dual-pane 11/16" dual-seal [[annealed] [tempered]] non-impact laminated glass [[clear] [[Advanced Low-E] [SunDefense Low-E] with Argon]] [[bronze] [gray] [green] Advanced Low-E [with argon]].
 – or –
•	Silicone-glazed 1" triple-seal insulating glass [[annealed] [tempered]] [[Advanced Low-E] [SunDefense™] [NaturalSun Low-E] with [argon]].
– or –
•	Impact-Resistant
•	Silicone-glazed 1" dual-seal impact-resistant insulating glass 1 SGP. [[tempered] [annealed]] exterior light is [[Advanced Low-E] [SunDefense] with argon] [clear] [bronze] [gray] [green]]. Laminated clear interior light.
– or –
•	Silicone-glazed 11/16" dual-seal impact-resistant insulating glass 1 [PVB]. [[tempered] [annealed]] exterior light is [[Advanced Low-E with argon] [clear]]. Laminated [clear] interior light, or [[tempered] [annealed]] exterior light is [[Advanced Low-E] [SunDefense] with argon] [clear]]. Laminated [[bronze] [gray] [green]] interior light.

Exterior
•	Exterior aluminum surfaces are finished with EnduraClad® multi-stage finish system.
•	Color is [Standard2] [custom2]. 
– or –
•	Exterior aluminum surfaces are finished with EnduraClad Plus 70% fluoropolymer-based multi-stage finish system. 
•	Color is [Standard2] [custom2]..
Interior
•	[Unfinished, ready for site finishing] [Factory-primed with one coat acrylic latex] [Pine: [Factory prefinished [paint] [stain] 2].
Hardware 
•	Finish of finger pull handle is [baked enamel, [Champagne] [White] [Brown]] [Satin Brass] [Satin Nickel] [Oil-Rubbed Bronze]. 
•	All vent units are available with left- or right-hand hinging.
•	SureLock® System—A single handle locking system operates positive-acting arms that reach out and pull the sash into a locked position: one installed on units 29" and smaller frame height, two unison operating locks installed on units over 29" frame height. 
•	Saldo Lock handle finish is [baked enamel, [Champagne] [White] [Brown] [Matte Black]] [Satin Brass] [Satin Nickel] [Oil-Rubbed Bronze].
•	Factory applied window opening control device included. Device allows window to open less than 4" with normal operation, with a release mechanism that allows the sash to open completely.
Optional Products
Grilles
•	Integral Light Technology® grilles
•	Interior grilles are [5/8”] [7/8"] [1-1/4"] [2"] square profile that are solid [pine] [mahogany] [douglas fir]. Interior surfaces are [unfinished, ready for site finishing] [factory primed] [pine: factory prefinished [paint] [stain] 2].
•	Exterior grilles are [5/8”] [7/8"] [1-1/4"] [2"] square profile that are extruded aluminum.
•	Patterns are [Traditional] [Prairie] [Top Row] [Cross].
•	Insulating glass contains non-glare spacer between the panes of glass.
•	Grilles are adhered to both sides of the insulating glass with VHB acrylic adhesive tape and aligned with the non-glare spacer.
– or –
•	Grilles-Between-the-Glass 3
•	Insulating glass contains 3/4" contoured aluminum grilles permanently installed between two panes of glass (exterior air-space on triple-pane insulating glass).
•	Patterns are [Traditional] [Prairie] [Cross] [Top Row].
•	Interior color is [Black] [White] [Brown4] [Fossil] [Harvest] [Cordovan] [Ivory] [Tan4] [Brickstone] [Putty4].
•	Exterior color5 is [standard]2
Hinged In-Swing Screen
•	InView™ Fiberglass Screen
•	Vinyl-coated 18/18 mesh fiberglass screen cloth complying with SMA 1201, set in an aluminum extruded frame fitted to inside of window, supplied complete with all necessary hardware.
•	Screen frame interior exposed surfaces are extruded aluminum with [White] [Brown] [Black] painted finish.
Hardware
•	Optional factory applied limited opening hardware available for vent units in stainless steel; nominal 3" opening.

(1) Insulating glass with argon is Low-E coated (except high altitude). All other insulating glass (including high altitude Low-E) is air-filled.
(2) Contact your local Pella sales representative for current color options.
(3) Available in clear, Low-E or obscure insulating glass.
(4) Tan, Brown or Putty Interior GBG colors are available in single-tone (Brown/Brown, Tan/Tan or Putty/Putty). Other interior colors are also available with Tan or Brown exterior.
(5) Appearance of exterior grille color will vary depending on Low-E coating on glass.
(6) Vivid View screen is not available when frame height is > 84" or when both frame width and frame height are > 48".