Pella® Reserve™ - Traditional Casement
Aluminum EnduraClad® Exterior
Detailed Product Description

Frame 
•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage. 
•	Interior exposed surfaces are [clear pine] [mahogany] [douglas fir]. Any curved member may have visible finger-jointed surfaces.
•	Exterior surfaces are clad with aluminum. 
•	Components are assembled with screws, staples and concealed corner locks
•	Overall frame depth is 5" (127mm) for a wall depth of 3-11/16" (94mm).
•	Optional factory-applied jamb extensions available between 3-13/16" (97mm) and 9-3/16" (233mm).
•	Optional factory-installed fold-out installation fins with flexible fin corners. 
•	Optional factory-applied EnduraClad® exterior trim.
Sash 
•	Select softwood, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage. 
•	Interior exposed surfaces are [clear pine] [mahogany] [douglas fir]. Any curved member may have visible finger-jointed surfaces.
•	Exterior surfaces are clad with extruded aluminum butt-jointed at all corners of the sash with through-stile construction and sealed. 
•	Corners mortised and tenoned, glued and secured with metal fasteners. 
•	Sash thickness is [1-13/16" (46mm) for 11/16"] [2-1/8" (54mm) for 1"] glazing.
•	Sash exterior profile is [ogee] [putty glaze], interior profile is ogee.
Weatherstripping 
•	Dual weatherstripping. 
•	Flexible santoprene material compressed between frame and sash for positive seal on all four sides. 
•	Secondary thermoplastic vulcanizate (TPV) leaf-type weatherstrip between edge of sash and frame on the vertical sides and bottom, and Santoprene® bulb-type weatherstrip on the top.
Glazing System1
•	Quality float glass complying with ASTM C 1036.
•	Silicone-glazed dual-pane 11/16" dual-seal insulating glass [[annealed] [tempered]], [[clear] [[Advanced] [SunDefense™] [SunDefense+] [NaturalSun] [NaturalSun+] [AdvancedComfort] Low-E [with argon]] [[bronze] [gray] [green] Advanced Low-E [with Argon]] [obscure] [Reflective Bronze] [Reflective Gray]. 
-or- 
•	Silicone-glazed dual-pane 1" dual-seal tempered spandrel glass [Lava Bronze Amber] [Black] [Ford Blue] [Symmetry Bronze] [Symmetry Gray] [Symmetry Green]. 
-or- 
•	Silicone-glazed dual-pane 11/16" dual-seal [[annealed] [tempered]] non-impact laminated glass [[clear] [[Advanced] [SunDefense] Low-E [with Argon]] [[bronze] [gray] [green] Advanced Low-E [with argon]]. 
– or –
•	Silicone-glazed 1” triple-pane, dual-seal insulating glass [[annealed] [tempered]] [[Advanced] [SunDefense™] [NaturalSun] Low-E [with argon]].
– or –
•	Impact-Resistant
•	Silicone-glazed 1" dual-seal impact-resistant insulating glass1 [SGP]. [[tempered] [annealed]] exterior light is [[Advanced] [SunDefense] Low-E with argon]] [clear] [bronze] [gray] [green]]. Laminated clear interior light.
– or –
•	Silicone-glazed 11/16" dual-seal impact-resistant insulating glass1 [PVB]. [[tempered] [annealed]] exterior light is [[Advanced Low-E with argon] [clear]]. Laminated [clear] interior light, or [[tempered] [annealed]] exterior light is [[Advanced] [SunDefense] Low-E with argon] [clear]]. Laminated [[bronze] [gray] [green]] interior light.
Exterior
•	Aluminum clad exteriors shall be finished with EnduraClad® protective finish, in a multi-step, baked-on finish.
•	Color is [standard] [custom]2.
– or –
•	Aluminum clad exteriors shall be finished with EnduraClad Plus protective finish with 70% fluoropolymer resin in a multi-step, baked-on finish 
•	Color is [standard] [custom]2.
Interior
•	[Unfinished, ready for site finishing] [factory primed with one coat acrylic latex] [factory prefinished [paint] [stain] 2].

Hardware 
•	Roto operator assembly
•	Steel worm gear sash operator with hardened gears.
•	Operator base is zinc die cast with painted finish. 
•	Operator linkage, hinge slide, and hinge arms are stainless steel. 
•	Exposed fasteners are stainless steel. 
•	Hardware shall exceed 1,000 hours salt spray exposure per ASTM B 117. 
•	All vent units are available with left- or right-hand hinging.
•	SureLock® System—A single handle locking system operates positive-acting arms that reach out and pull the sash into a locked position: one operating lock installed on units with frame height 29" and less, two unison operating locks installed on units with frame height over 29". 
•	Style of hardware is [Standard integrated fold-away crank and standard lock handle with [baked enamel [Champagne] [White] [Brown] [Matte Black]] [Satin Brass] [Satin Nickel] [Oil-Rubbed Bronze] hardware finish].
– or –
•	[Antiek fold-away crank and Antiek lock handle with [baked enamel [Champagne] [White] [Brown] [Matte Black]] [Satin Brass] [Satin Nickel] [Oil-Rubbed Bronze] [distressed bronze] [distressed nickel] hardware finish].
Optional Products
Grilles
•	Integral Light Technology® grilles
•	Interior grilles are [5/8”] [7/8"] [1-1/4"] [2"] ogee profile that are solid [pine] [mahogany] [douglas fir]. Interior surfaces are [unfinished, ready for site finishing] [factory primed] [pine: factory prefinished [paint] [stain] 2].
•	Exterior grilles are [5/8” putty glaze profile] [7/8" [putty glaze] [ogee] profile] [1-1/4" [putty glaze] [ogee] profile] [2" ogee profile] that are extruded aluminum.
•	Patterns are [Traditional] [Prairie] [Top Row] [Cross] [New England] [Victorian] [Simulated French].
•	Insulating glass contains non-glare spacer between the panes of glass.
•	Grilles are adhered to both sides of the insulating glass with VHB acrylic adhesive tape and aligned with the non-glare spacer.
– or –
•	Grilles-Between-the-Glass 3
•	Insulating glass contains 3/4" contoured aluminum grilles permanently installed between two panes of glass (exterior air-space on triple-pane insulating glass).
•	Patterns are [Traditional] [Prairie] [Cross] [Top Row].
•	Interior color is [Black] [White] [Brown4] [Fossil] [Harvest] [Cordovan] [Ivory] [Tan4] [Brickstone] [Putty4].
•	Exterior color5 is [standard]2.
Screens
•	InView™ Screens
•	Vinyl-coated 18/18 mesh fiberglass screen cloth complying with the performance requirements of SMA 1201, set in aluminum frame fitted to inside of window, supplied complete with all necessary hardware.
•	Screen frame finish is [baked enamel [Champagne] [White] [Brown] [Black]] [Wrapped in wood veneer, factory prefinished stain to match interior finish].
– or –
•	Rolscreen® Soft-close Retractable Screen (for rectangular units only) 
•	InView™ Screen cloth, self-storing, rolling, black vinyl-coated 18/18 mesh fiberglass screen cloth complying with ASTM D 3656 and the performance requirements of SMA 1201 mounted behind overhead cover.
•	Cover finish is [factory prefinished paint] [[pine] [mahogany] [douglas fir] veneer wrapped over extruded aluminum with factory prefinished [stain] [paint]2].
•	Guides are aluminum extrusion with [[pine] [mahogany] [douglas fir] veneer wrapped over extruded aluminum with factory prefinished [stain] [paint] 2].
Hardware
•	Optional factory applied limited opening hardware available for vent units in stainless steel; nominal 3" opening.
•	Optional factory applied window opening control device. Device allows window to open less than 4” with normal operation, with a release mechanism that allows the sash to open completely. Complies with ASTM F2090-17.

(1) Low-E coated insulating glass is argon-filled (except high altitude). All other insulating glass (including high altitude Low-E) is air-filled.
(2) Contact your local Pella sales representative for current designs and color options.
(3) Available in clear or Low-E insulating glass with argon, and obscure insulated glass.
(4) Tan, Brown and Putty Interior GBG colors are available in single-tone (Brown/Brown, Tan/Tan or Putty/Putty). Other interior colors are also available with tan or brown exterior.
(5) Appearance of exterior grille color will vary depending on Low-E coating on glass.