Pella® Reserve – Traditional Precision-Fit® Double-Hung Windows
Wood Exterior
Detailed Product Description

Frame 
•	Select softwood, water-repellent, preservative-treated with EnduraGuard® triple wood protection in accordance with WDMA I.S.-4. EnduraGuard triple protection formula includes water-repellency, three active fungicides and an insecticide applied to the frame.
•	Interior exposed surfaces are [pine] [mahogany].
•	Exterior surfaces are clad with aluminum. 
•	Pocket depth is 3-1/4" (83mm).
•	Vinyl Jamb liner includes wood / clad inserts.
Sash 
•	Select softwood, water-repellent, preservative-treated with EnduraGuard triple wood protection in accordance with WDMA I.S.-4. EnduraGuard triple protection formula includes water-repellency, three active fungicides and an insecticide applied to the sash. 
•	Interior exposed surfaces are [pine] [mahogany].
•	Exterior surfaces are [pine] [mahogany]. 
•	Sash thickness is 1-13/16" (46mm).
•	Sash exterior profile is putty glaze, interior profile is ogee.
•	Upper sash has surface-mounted wash locks.
•	Lower sash has concealed wash locks in lower check rail.
•	Sashes tilt for easy cleaning.
Weatherstripping 
•	Water-stop Santoprene-wrapped foam at head and sill. 
•	Thermoplastic elastomer bulb with slip-coating set into lower sash for tight contact at check rail.
•	Kerf mounted bristle weatherstrip at sill.
•	Vinyl-wrapped foam inserted into jamb liner to seal against sides of sash.
Glazing System
•	Quality float glass complying with ASTM C 1036.
•	Custom and high altitude glazing available.
•	Silicone-glazed 11/16" dual-seal insulating glass [[annealed] [tempered]] [[clear] [[Advanced] [SunDefense™] [SunDefense+] [AdvancedComfort] [NaturalSun] [NaturalSun+] Low-E [with argon]] [[bronze] [gray] [green] Advanced Low-E with argon].
Exterior Sash
•	[Pine: factory primed with one coat acrylic latex] [Mahogany: [factory primed with one coat acrylic latex] [Unfinished, ready for site finishing]].
Interior
•	[Unfinished, ready for site finishing] [factory primed with one coat acrylic latex] [pine: factory prefinished [paint] [stain] 2].
Hardware 
•	Galvanized block-and-tackle balances are connected to self-locking balance shoes which are connected to the sashes using zinc die cast terminals and concealed within the frame.
•	Sash lock is [standard] [historic spoon-style]. Two sash locks on units with make width 37" and greater.
•	Optional Sash lift furnished for field installation. Two lifts on units with make width 37" and greater.
•	Hardware finish is [baked enamel [Champagne] [White] [Brown] [Matte Black]] [satin brass] [satin nickel] [oil-rubbed bronze] [distressed bronze] [distressed nickel].

Optional Products
Grilles
•	Integral Light Technology® grilles
•	Interior grilles are [5/8”] [7/8"] [1-1/4"] ogee profile that are solid [pine] [mahogany]. Interior surfaces are [unfinished, ready for site finishing] [factory primed] [pine: factory prefinished [paint] [stain] 2].
•	Exterior grilles are [5/8”] [7/8"] [1-1/4"] putty glaze profile [pine] [mahogany], water repellent, preservative-treated in accordance with WDMA I.S.-4, and are factory primed.
•	Patterns are [Traditional] [Prairie] [Top Row] [New England] [Victorian].
•	Insulating glass contains non-glare spacer between the panes of glass.
•	Grilles are adhered to both sides of the insulating glass with VHB acrylic adhesive tape and aligned with the non-glare spacer.
– or –
•	Grilles-Between-the-Glass 3
•	Insulating glass contains 3/4" contoured aluminum grilles permanently installed between two panes of glass.
•	Patterns are [Traditional] [9-Lite Prairie] [Cross] [Top Row]
•	Interior color is [Black] [White] [Brown4] [Fossil] [Harvest] [Cordovan] [Ivory] [Tan4] [Brickstone] [Putty4].
•	Exterior color5 is [standard2].
Screens
•	InView™ Screens
•	[Half-Size] [Full-Size] black vinyl-coated 18/18 mesh fiberglass screen cloth complying with the performance requirements of SMA 1201, set in a [standard roll form] [premium extruded] aluminum frame fitted to outside of window, supplied complete with all necessary hardware.
•	Spreader bar placed on units > 37" width or 64-1/4" make height.
•	Screen frame finish is baked enamel.
Hardware
•	Optional factory applied limited opening device available for vent units in stainless steel; nominal 3-3/4" opening. Limiting device concealed from view.
•	Optional factory applied window opening control device available.  Device allows window to open less than 4” with normal operation, with a release mechanism that allows the sash to open completely. Complies with ASTM F2090-10.

(1) Low-E coated insulating glass is argon-filled (except high altitude). All other insulating glass (including high altitude Low-E) is air-filled.
(2) Contact your local Pella sales representative for current color options.
(3) Available in clear or Low-E insulating glass only.
(4) Tan, Brown and Putty Interior GBG colors are available in single-tone (Brown/Brown, Tan/Tan or Putty/Putty). Other interior colors are also available with Tan or Brown exterior.
(5) Appearance of exterior grille color will vary depending on Low-E coating on glass.