Pella® Entry Door Systems
In-Swing/Out-Swing Composite Frames
Detailed Product Descriptions

Frame (Composite) 
•	Exterior surfaces are a multi-part composite material at the head and jambs. 
•	Color is [factory applied] [factory applied [stain finish 1] [paint finish 1]].2 When frame gets a stain finish, material will be a wood-grained material look, most closely resembling a Mahogany grain. 
•	Interior surfaces are composite [factory-primed] [stain-grade] [factory [stained finish 1] [painted finish 1]] to match exterior finish. 
•	Extruded thermally broken aluminum sill is [mill finish] [black]. With PVC threshold. 
•	Available in 4-9/16", 5-1/4" and 6-9/16" Wall depths 
•	Optional 20-minute fire rated frame is Warnock Hersey labeled 3. 
Door Panels (Fiberglass Units)
•	Fiberglass exterior and interior skins with CFC-free foam insulating core. 
•	Square-edged top and bottom rails. 
•	21" solid wood lock block reinforces latch and deadbolt installations [oak] [mahogany] [Flush Glazed] [all 96"]. 12" solid wood lock block reinforces latch and deadbolt installations [Smooth] 
•	Reinforcement available for Commercial hardware on out-swing panels (not available in fiberglass 2 Panel Square, 2 Panel Arch, or 2 Panel Arch Plank). 
•	Panel thickness is 1-3/4" (44.45 mm). 
•	Fiberglass grain is [Mahogany] [Oak] [Fir] [Smooth]. 
•	Interior and exterior surfaces is [unfinished] [factory applied [stain finish 1] [paint finish 1]].2 
•	Unfinished panel skin color is [Beige [Oak] [Mahogany] [Fir] [Smooth]]. 
•	Minimum of 0.075 skin thickness. 
Door Panels (Steel Units)
•	24-gauge galvanized steel skins on exterior and interior with CFC-free foam insulating core.
•	Bull nosed composite lock stile and finger jointed hinge side stile. 
•	Composite bottom rail. 
•	PVC top rail and stiles with LVL wood beneath it. 
•	12" solid wood lock block reinforces latch and deadbolt installations 
•	Panel thickness is 1-3/4" (44.45 mm). 
•	Interior and exterior surfaces are [factory primed] [factory applied paint finish 1]. 
•	Optional 20-minute fire rated solid panels are Warnock Hersey labeled3.
Weatherstripping 
•	Dual-durometer extruded polymer [In-Swing: along perimeter of door frames and along the bottom of door panels] [Out-Swing: along perimeter of door frames].
•	Compression type foam filled weatherstrip at head and jambs. 
•	Dual durometer extruded polymer with bulb at bottom rail of door panel will contact threshold and include drip. 
Glazing System
•	Quality float glass complying with ASTM C 1036. 
•	Glazing rims are acrylonitrile styrene acrylate. 
•	Dual-seal insulating glass assemblies consisting of tempered: [multi-layer Low-E coated 4] or decorative panel designs of [Huxley] [Floris] [Avoca] [Pel] [Story] [Lucas] [Tune] [Lovilia] [Danbury] [Cross Reed] [Chord] [Double Water] [Narrow Reed] [Pear] [Satin Etch] shall be installed into high performance glazing frames or glazed rim on Craftsman units. 
•	Impact-Resistant 
•	1" IG dual-seal impact-resistant insulating glass PVB. Tempered glass is [Low- E] or decorative panel designs of [Avoca] [Tune] [Chord] [Pear] [Satin Etch]. 

        

 
Hardware and Hardware Prep 
Hinges
•	Hinges are [In-Swing: [Standard Steel Ball Bearing] [Steel Spring (fire rated doors only, on top and bottom hinge placements – 2 steel spring hinges total)]] three (3) per door panel on 6' 8" and 7' 0" panel heights; four (4) per door panel on 8' 0" heights for operable units] [Out-Swing: [Standard Steel Ball Bearing] [Steel Spring (fire rated doors only, on top and bottom hinge placements – 2 steel spring hinges total)] three (3) per door panel on 6' 8" and 7' 0" panel heights; four (4) per door panel on 8' 0" heights for operable units]. 
•	Hinge finish is [Brass] [Satin Nickel] [Matte Black] [Stainless Steel]. 
•	All operable units are available with left- or right-hand hinging. 
Standard Hardware Prep
•	Each door panel is [no bore] [factory-prepped for 2-1/8" (54 mm) latch bore] [factory-prepped for 2-1/8" (54 mm) latch bore and 2-1/8" deadbolt, 5-1/2" (140 mm) on center, Impact door over 7'0" in height has 10-1/2" (241.3 mm) on center]. Backset is [2-3/8" (60 mm)] [2-3/4" (70 mm)]. 
•	Optional interior and exterior cylindrical passage hardware is [PVD Brass] [PVD Satin Nickel] [Oil-Rubbed Bronze] [Distressed Nickel] with Kwikset 5-pin configured keyway pinlock cylinder. 
Multi-point Hardware Prep
•	Multi-point lock mechanism includes stainless steel face plate. 
•	Multi-point lock handle set hardware, with Kwikset 5-pin configured keyway, is [Brass] [Satin Nickel] [Oil-Rubbed Bronze]. 
Frame Reinforcement
•	Single doors without sidelights include a 24-gauge steel jamb reinforcement plate on the backside of the deadbolt bore, when the double bore option is chosen. 

Optional Products
Grilles and Blinds
•	Grilles-Between-the-Glass 
•	Insulating glass contains 5/8" flat aluminum grilles permanently installed between two panes of glass. 
•	Available only on glazed [Flush Glazed units] [Craftsman units]. 
•	Grille patterns are [Traditional] [Prairie] [Top Row]. 
•	Grilles are factory pre-finished [[White] interior] [[White] [Black] exterior]. 
– or –
•	Simulated-Divided-Light grilles
•	Grilles are permanently bonded to the interior and exterior glass surface. 
•	Grilles are expanded PVC. 
•	Surfaces are [unfinished, ready for site finishing] [factory finished to match interior and exterior finish]. 
•	Available only on units glazed with [Low-E insulated glass] [textured and obscure glass]. 
•	Grille patterns are [Traditional] [Prairie] [Top Row (Flush Glazed units only)]. 
•	Grille profiles are [1-1/8" Contour] [3-1/2" Flat (Flush Glazed Full Light only)]. 
– or – 
•	Fixed Grilles 
•	Grilles are expanded ASA. 
•	Surfaces are [unfinished, ready for site finishing] [factory finished to match interior and exterior finish]. 
•	Available only on units glazed with [Low-E insulated glass] [textured and obscure glass]. 
•	Grille pattern is [Traditional]. 
•	Grille contour is [7/8"].
– or –
•	Blinds-Between-the-Glass
•	White aluminum blinds sealed between dual-pane clear insulating glass.
•	Cordless raise, lower and tilt one handed operation. Operator mounted on interior right-hand side of panel/sidelight.
Decorative Accents
•	Dentil Shelf (available on Craftsman doors only)
•	Shelf is factory applied.

(1) Contact your local Pella sales representative for current color options. 
(2) Smooth grain doors are not available in factory applied stain finish.
(3) Not available in double-panel widths.
(4) Low-E Not available on ¾ Oval Light or ¾ Deluxe Oval Light glazing.