Pella® Reserve - Traditional Push Out Casement
Wood Exterior
Detailed Product Descriptions

Frame 
•	Select woods, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are [Pine] [Mahogany] (standard rectangular windows only). Any curved member may have visible finger-jointed surfaces.
•	Exterior surfaces are [Pine: primed] [Mahogany: [primed] [ready-to-stain]]. 
•	Overall frame depth is 4-3/8" (111 mm) for a wall depth of 4-3/16" (106 mm).
•	Optional factory-applied jamb extensions available between 4-9/16" (116 mm) and 7-3/16" (183 mm) wall depths, with Pella's standard wood exterior trim.
Sash 
•	Select woods, immersion treated with Pella’s EnduraGuard® wood protection formula in accordance with WDMA I.S.-4. The EnduraGuard formula includes three active ingredients for protection against the effects of moisture, decay, stains from mold and mildew. Plus, an additional ingredient adds protection against termite damage.
•	Interior exposed surfaces are [Pine] [Mahogany] (standard rectangular windows only). Any curved member may have visible finger-jointed surfaces.
•	Exterior surfaces are [Pine: primed] [Mahogany: [primed] [ready-to-stain]].  
•	Corners mortised and tenoned, glued and secured with metal fasteners. 
•	Sash thickness is 1-13/16" (46 mm).
•	Exterior sash profile is putty glaze, interior sash profile is ogee. 
Weather Stripping 
•	Dual weather stripping. 
•	Flexible santoprene material compressed between frame and sash for positive seal on all four sides. 
•	Secondary polyvinyl chloride leaf-type weather strip between edge of sash and frame.
Glazing System1
•	Quality float glass complying with ASTM C 1036.
•	Silicone-glazed 11/16" dual-seal insulating glass [[annealed] [tempered]] [[clear] [Advanced Low-E coated with argon]] [SunDefense™ Low-E with Argon] [AdvancedComfort Low-E] [NaturalSun Low-E] [[bronze] [gray] [green] air-filled Advanced Low-E coated]].
•	Custom and high altitude [with argon] glazing available. 
Interior 
•	[Unfinished, ready for site finishing] [primed with one coat acrylic latex] [Pine: [Factory prefinished [paint] [stain] 3].
Hardware 
•	Finish of finger pull handle is [baked enamel, [Champagne] [White] [Brown]] [Satin Brass] [Satin Nickel] [Oil-Rubbed Bronze]. All vent units are available with left- or right-hand hinging.
•	SureLock® System—A single handle locking system operates positive-acting arms that reach out and pull the sash into a locked position: one operating lock installed on units with frame height 29" and less, two unison operating locks installed on units with frame height over 29". 
•	Style of hardware is [Standard standard lock handle with [baked enamel [Champagne] [White] [Brown] [Matte Black]] [Satin Brass] [Satin Nickel] [Oil-Rubbed Bronze] hardware finish].
– or –
•	[Antiek lock handle with [baked enamel [Champagne] [White] [Brown] [Matte Black]] [Satin Brass] [Satin Nickel] [Oil-Rubbed Bronze] [distressed bronze] [distressed nickel] hardware finish].
•	Factory applied window opening control device included. Device allows window to open less than 4" with normal operation, with a release mechanism that allows the sash to open completely.
Optional Products
Grilles
•	Interior grilles are [5/8”] [7/8"] [1-1/4"] [2"] ogee profile that are solid [pine] [mahogany]. Interior surfaces are [unfinished, ready for site finishing] [factory primed] [pine: factory prefinished [paint] [stain] 3].
•	Exterior grilles are solid [5/8” putty profile] [7/8" [putty] [ogee] profile] [1-1/4" [putty] [ogee] profile] [2" ogee profile] that are [pine] [mahogany]. Exterior surfaces are water repellent, preservative-treated in accordance with WDMA I.S.-4, and are [unfinished, ready for site finishing] [factory primed]. 
•	Patterns are [Traditional] [Prairie] [Top Row] [Cross] [New England] [Victorian] [Simulated French].
•	Insulating glass contains non-glare spacer between the panes of glass.
•	Grilles are adhered to both sides of the insulating glass with VHB acrylic adhesive tape and aligned with the non-glare spacer.
– or –
•	Grilles-Between-the-Glass2 
•	Insulating glass contains 3/4" contoured aluminum grilles permanently installed between two panes of glass.
•	Patterns are [Traditional] [Prairie] [Cross] [Top Row] [Custom – Equally Divided].
•	Interior color is [Black] [White] [Brown4] [Fossil] [Harvest] [Cordovan] [Ivory] [Tan4] [Brickstone] [Putty4].
•	Exterior color5 is [standard3].
Hinged In-Swing Screens
•	InView™ Fiberglass Screen
•	Vinyl-coated 18/18 mesh fiberglass screen cloth complying with SMA 1201, set in an aluminum extruded frame fitted to inside of window, supplied complete with all necessary hardware.
•	Screen frame interior exposed surfaces are extruded aluminum with [Artisan Greige] [Skyline Gray] [White] [Brown] [Black] painted finish.
Hardware
•	Optional historical visible stay bar available in [Satin Brass] [Satin Nickel] 
[Oil-Rubbed Bronze].
•	Optional factory applied limited opening hardware available for vent units in stainless steel; nominal 3" opening.
Sensors
•	Optional factory installed integrated security sensors available in vent units.

(1) Insulating glass with argon is Low-E coated. All other insulating glass is air-filled.
(2) Available in clear, Low-E and obscure insulating glass.
(3) Contact your local Pella sales representative for current color options.
(4) Tan, brown and putty Interior GBG colors are available in single-tone (brown/brown, tan/tan or putty/putty). Other interior colors are also available with tan or brown exterior.
(5) Appearance of exterior grille color will vary depending on Low-E coating on glass.