Pella Hurricane Shield Series
Awning
Detailed Product Description

Frame
•	Overall frame depth: 3-1/4" on all frame types.
•	Frame members are mitered and heat-fused to provide a fully welded corner assembly. Sill is fitted with weeps.
•	Frame: [1-1/8" setback for nail fin for 2-1/8" wall depth] [Block frame for 3-1/4" wall depth] [Integral 5/8" flange for 3" wall depth]. 
•	 Interior and exterior frame surfaces are extruded rigid PVC.
Sash
•	Sash members are extruded, rigid PVC.
•	Sash members are mitered and heat-fused to provide a fully welded corner assembly.
•	Contains sealed insulating glass.
Weatherstripping
•	Vent units include weatherstripping around the sash perimeter with a fin type, pile and an extruded bulb weatherstrip.
Glazing System
•	Quality float glass complying with ASTM C1036.
•	Exterior face glazed sealed insulating glass.
•	Dual-Pane insulating glass [[annealed] [tempered]] [[Advanced] [Coastal] [SunDefense™] [Neat, SunDefense] [Obscure, SunDefense] Low-E coated [with Argon]] [Obscure] [Gray] [Blue] [Bronze].
Interior / Exterior
•	All window frame and sash members are [[White] [Bronze] with integral color extruded throughout the profiles] [Bronze exterior, white integral on interior]. Exterior, consisting of a solar reflective coating exceeding AAMA 613 test requirements, with White integral color extruded throughout the profiles on the interior]. 
•	All exposed PVC surfaces are smooth, glossy and uniform in appearance.
Hardware
•	Dual lock with dual handles. Lock handles on jambs. Lock tie-bars are stainless steel.
•	High quality [steel] [stainless steel] dual-arm roto-operator with fold down crank handle located on sill.
•	Hinge arms are [steel] [stainless steel].
•	Corrosion-resistant fasteners of PVC-compatible material.
•	Hardware finish is [White] [Bronze]. 
Screens
•	Set in aluminum frame and fitted to interior of window.
•	Screen frame finish is baked enamel, color to match interior. 
•	Supplied complete with all necessary hardware.
•	InView™ Screens
•	Black vinyl coated 18/18 mesh fiberglass screen cloth complying with SMA 1201. 
Optional Products	
Grilles
•	Grilles-Between-the-Glass
•	Dual-Pane Insulating glass contains [[3/4"] [1"] contoured] [5/8" flat] aluminum grilles permanently installed between two panes of glass. 
•	Patterns are [Traditional] [6-Lite Prairie] [9-Lite Prairie] [Top Row1]. 
•	Interior grille color matches interior frame. 
•	Exterior grille color matches exterior frame. 

•	Exterior Applied Grille with Grilles-Between-the-Glass.
•	7/8" grilles permanently bonded to the exterior of glass with 1" contour grilles permanently installed between two panes of glass. 
•	Patterns are [Traditional] [9-Lite Prairie]. 
•	Grilles match color of interior and exterior frame. 
Hardware
•	Optional limited opening hardware available for vent units in [White] [Bronze] extruded vinyl to match the unit; nominal 3" opening.
•	Optional window opening control device available for field installation. Device allows window to open less than 4" with normal operation, with a release mechanism that allows the sash to open completely. Complies with ASTM F2090-10.

(1) Top Row is only available with 5/8" flat grilles between-the-glass.