Pella Hurricane Shield Series
Multi-Slide Patio Door
Detailed Product Description

Frame
•	Overall frame depth: 6".
•	Frame members are mitered knock-down. Sill is fitted with weeps.
•	Frame: Block frame 6" wall depth] 
•	Interior and exterior frame surfaces are extruded rigid PVC.
Door Panels
•	Door Panel consists of extruded, rigid uPVC.
•	Panel members are mitered and heat-fused to provide a fully welded corner assembly. 
•	Vent panel is fully operable for ventilation. 
•	Vent panels have two adjustable rollers, set on an extruded aluminum track. 
•	Contains sealed insulating glass. 
Weatherstripping
•	Fin-type pile around perimeter of panels.
Glazing System
•	Quality fully-tempered float glass complying with ASTM C 1036. 
•	Exterior face-glazed sealed insulating glass. 
•	Dual-Pane insulating glass with argon [Advanced Low-E coated] [Turtle Glass] [SunDefense™ Low-E coated] [Neat, SunDefense], [Obscure, SunDefense] [Obscure] [Bronze] [Gray] [Blue]. 
Interior / Exterior
•	All frame and panel members are White with integral color extruded throughout the profiles, consisting of a solar reflective coating exceeding AAMA 613 test requirements. 
•	All exposed PVC surfaces are smooth, glossy and uniform in appearance.
Hardware
•	Interior handle and thumblock; finish is White. 
•	Exterior handle finish is Black. 
•	Keylock with K-keyway cylinder. Finish is Chrome. 
•	All fasteners are a corrosion-resistant material compatible with PVC. 
•	Multi-point lock, stainless steel. 
•	Door rollers are adjustable, permanently sealed, corrosion resistant stainless steel, ball bearing rollers. 
Screens
•	Full-size Fiberglass sliding screen with black vinyl coated 18/18 mesh fiberglass screen cloth complying with ASTM D 3656 and SMA 1201 set in an extruded aluminum frame. 
•	Supplied with four self-adjustable rollers, latch and latch handle. 
•	Frame of screen matches exterior frame color 
Optional Products	
Grilles
•	Grilles-Between-the-Glass
•	Insulating glass contains [3/4"] [1"] contoured or 5/8" flat aluminum grilles permanently installed between two panes of glass.
•	Patterns are [Traditional] [9-Lite Prairie].
•	Grille color matches frame finish 1..  

1) Only 5/8" flat grilles are available in two-tone finishes