Vinyl Windows and Doors Manufactured by Pella Corporation 
Fixed Frame Window – East and West Regions 
Detailed Product Descriptions

EAST REGION
Frame
•	Overall frame depth is [2-9/16” new construction frame with integral fin and J-channel] [2-11/16" [new construction frame [with integral nailing fin] [with integral nailing fin and J-channel]] [2-11/16” replacement frame] [with 1/2” integral flush flange (Florida region only)]] [3-1/4" replacement frame].
•	Frame members are extruded, rigid uPVC.
•	Frame members are mitered and heat-fused to provide a fully welded corner assembly.
Glazing 
•	Quality float glass complying with ASTM C1036
•	Exterior face glazed 3/4" sealed insulating glass.
•	[Clear] [[Advanced] [SunDefenseTM] [SunDefense+] [NaturalSun] [NaturalSun+] [Bronze, Advanced] Low-E coated [with Argon]]; [Obscure] [Tempered].
Interior / Exterior
•	All window frame members are an integral color extruded throughout the profiles.
•	All exposed uPVC surfaces are smooth, glossy and uniform in appearance.
•	East Region Finish color [White] [Almond] [Fossil] (all frame types).
Optional Products	
•	Grilles-Between-the-Glass
•	Insulating glass contains [[3/4"] [1"] contoured] aluminum grilles permanently installed between two panes of glass.
•	Grilles match color of frame. 
•	Factory applied primed wood jamb extension for [4-9/16"] [6-9/16"] wall depth available on 2-11/16” fin frames.

WEST REGION
Frame
•	Overall frame depth is [ 2-11/16" replacement frame] [2-11/16" new construction frame with integral fin] [2-11/16” replacement frame with integral flush flange].
•	Frame members are extruded, rigid uPVC.
•	Frame members shall be mitered and electrically heat fused to provide a fully welded corner assembly.
Glazing 
•	Quality float glass complying with ASTM C1036
•	Exterior face glazed 3/4" sealed insulating glass.
•	[Clear] [[Advanced] [SunDefenseTM] [SunDefense+] [NaturalSun] [NaturalSun+] [Advanced Comfort] Low-E [with argon]] [Standard Obscure1 [Rain]] [Tempered] [High Altitude [with argon]].
Interior / Exterior
•	All window frame members are an integral color extruded throughout the profiles.
•	All exposed uPVC surfaces are smooth, glossy and uniform in appearance.
•	West Region Finish color [White (all frame types)] [[Almond] [Fossil] (Nail Fin frame only)].
Optional Products	
•	Grilles-Between-the-Glass
•	Insulating glass contains [5/8" flat] [3/4" contoured] aluminum grilles permanently installed between two panes of glass.
•	Grilles match color of frame. 

(1) Obscure glass not available with Bronze Advanced, SunDefense+ or NaturalSun+ Low-E IG.