Vinyl Windows and Doors Manufactured by Pella Corporation
Radius Shape Windows - East and West Regions
Detailed Product Description

Frame
•	Overall frame depth: [2-11/16" [new construction frame with integral nailing fin [and J-channel (East region only)] [integral flush flange (Florida region only)]]; [3-1/4” replacement frame (East region only)]; [3-1/4" new construction frame with integral nailing fin (East region only)].
•	Frame members are extruded rigid uPVC.
•	Frame members are mitered and heat-fused to provide a fully welded corner assembly. 
Glazing System
•	Quality float glass complying with ASTM C 1036.
•	Exterior face-glazed 3/4" sealed insulating glass.
•	[Clear] [[Advanced] [SunDefense™] [SunDefense+] [NaturalSun] [NaturalSun+] [Advanced Comfort (West region only)] [Bronze, Advanced (East Region only)] Low-E [with Argon]]; [Clear] [NaturalSun Low-E] [Obscure1] [Tempered] [Standard Obscure1 [rain] (West region only)] [High altitude [with argon] (West region only)].
Interior / Exterior
•	All window frame members have an integral color extruded throughout the profiles.
•	All exposed uPVC surfaces are smooth, glossy and uniform in appearance. 
•	East Region Finish color [White] [Almond] [Fossil] (all frame types); West Region Finish color [White (all frame types)] [[Almond] [Fossil] (Nail Fin frame only)].
Optional Products	
•	Grilles-Between-the-Glass
•	Insulating glass contains [3/4" contoured (East or West)] [5/8" flat (West)] aluminum grilles permanently installed between two panes of glass.
•	Grilles match color of interior and exterior frame.
•	Factory applied primed wood jamb extension for [4-9/16"] [6-9/16"] wall depth, for 2-11/16” new construction frame East region.

(1) Obscure glass not available with Bronze Advanced, SunDefense+ or NaturalSun+ Low-E IG.