Vinyl Windows and Doors Manufactured by Pella Corporation
Sliding Window – East and West Regions
Detailed Product Description

Frame
•	Overall frame depth is [2-11/16” [new construction frame with integral nailing fin [and J-channel]] [replacement frame [with integral flush flange (Florida region only)]].
•	Frame members are extruded, rigid uPVC [with optional foam insulation1].
•	Frame members are mitered and heat-fused to provide a fully welded corner assembly.
Sash
•	Sash members are extruded, rigid uPVC [with optional foam insulation1].
•	Sash members are mitered and heat-fused to provide a fully welded corner assembly.
Weatherstripping
•	Fin-type pile around the perimeter of the vent sash.
Glazing System2
•	Quality float glass complying with ASTM C 1036.
•	Exterior face-glazed 3/4" sealed insulating glass.
•	[[Clear] [Advanced] [SunDefense™] [SunDefense+] [NaturalSun] [NaturalSun+] [Advanced Comfort(West region only)] [Bronze, Advanced (East Region only)] Low-E [with argon]]; [Clear] [NaturalSun Low-E] [Obscure (East region only)] [Standard Obscure [Fern (West region only)] [Rain] [Tempered] [High altitude [with argon] (West region only)].
Interior / Exterior
•	All window frame members are an integral color extruded throughout the profiles.
•	All exposed uPVC surfaces are smooth, glossy and uniform in appearance.
•	East Region Finish color [White] [Almond] [Fossil] (all frame types); West Region Finish color [White (all frame types)] [[Almond] [Fossil] (Nail Fin frame only)].
Hardware
•	Lock is factory-installed zinc die cast, self-aligning, cam-action lock located on the meeting rail factory pre-finished to match unit.
•	Vent unit sash is equipped with two nylon roller housings containing two nylon rollers each.
•	One sash lock is installed on all units.
Optional Products	
•	Factory applied primed wood jamb extension for [4-9/16"] [6-9/16"] wall depth, for 2-11/16” fin frame East region units only. 
Grilles
•	Grilles-Between-the-Glass
•	Insulating glass contains [3/4" contoured (East or West)] [5/8" flat (West only)] aluminum grilles permanently installed between two panes of glass.
•	Grilles match color of interior and exterior frame.
Hardware
•	Optional limited opening device available for field installation for all venting units; nominal 3" opening. Off-white rubber bumper to be installed at the head of the venting unit.
•	Optional window opening control device available for field installation. Device allows window to open less than 4” with normal operation, with a release mechanism that allows the sash to open completely. Complies with ASTM F2090-10.
Screens
•	Half-size with black vinyl coated 18/14 mesh fiberglass screen cloth complying with L-S-125B and ANSI SMA 1004.
•	Set in aluminum frame and fitted to exterior of window.

(1) Foam insulation inserts are not available with clear glazing.
(2) SunDefense+ and NaturalSun+ are only available with argon fill, and are not available for obscure glass.