Pella® Vinyl Windows and Doors Complimentary Products 
Pella 250 Series Premium Hinged Patio Doors (In-Swing and Out-Swing)
Detailed Product Description

Frame
•	Overall frame depth: 5-1/4”.
•	Frame members are mitered and heat-fused fully welded.
•	Frame: [1” setback for nail fin for 4-1/4” wall depth and 1-3/8” setback for nail fin for 3-7/8” wall depth] [Block Frame for 5-1/4” wall depth] [Flush Flange for 5” wall depth].
•	Sill options: [Standard] [Low-profile].
•	Interior and exterior frame surfaces are extruded rigid uPVC.
Door Panel
•	3-3/4” x 1-3/4" vinyl panel with internal aluminum reinforcement.
•	Door panel consists of extruded, rigid uPVC.
•	Panel members are mitered and heat-fused to provide a fully welded corner assembly.
•	Contains sealed insulating glass.
Weatherstripping
•	Foam-backed weatherstripping on the main frame.
Glazing System
•	Interior face-glazed sealed insulating glass. 
•	Standard Dual-Pane tempered glass, with optional Triple-Pane upgrade.
•	7/8” Dual-Pane insulating glass [Advanced Low-E coated [with argon]] [SunDefense™ Low-E coated [with argon]] [High Altitude1].
-or-
•	1-1/4” Triple-Pane insulating glass [SunDefense™ Low-E coated [with argon]] [High Altitude1].
Interior / Exterior
•	Frame and panel members are [[White] [Beige] with integral color extruded throughout the profiles]
-or-
•	Brown laminate exterior, with White integral color extruded throughout the profiles on the interior.
-or-
•	Black laminate exterior, with optional [Black] laminate interior or White integral color extruded throughout the profiles on the interior."
•	Sill: [[Bronze Anodized] [Mill]] finish options.
•	All exposed PVC surfaces are smooth, glossy and uniform in appearance.
Hardware
•	Interior handle and thumb-lock; finish is [[White] [Black] [Satin Nickel]].
•	Exterior handle with optional keylock; finish is [[White] [Black] [Satin Nickel]].
•	Multipoint locking hardware [Stainless Steel] located on both active and inactive panels. 
•	Adjustable contemporary hinges; finish is [[White] [Bronze] [Silver Coated] [Black]].

(1) Dual-Pane IG High Altitude glazing is only available without Argon. Triple-Pane IG High Altitude glazing is only available without Argon.