Pella® Vinyl Windows and Doors 
Pella 250 Series Classic Sliding Patio Door
Detailed Product Description

Frame
•	Overall frame depth: 5".  
•	Frame members are mitered and heat fused to provide a fully welded corner assembly. Sill is fitted with weeps.
•	Frame: [1-1/8" setback nail fin for 3-7/8" wall depth] [Block frame for 5" wall depth] [Double Wall Flush flange for 4-3/4" wall depth] [Integral 5/8 flange for 4-3/4" wall depth]. 
•	Interior and exterior frame surfaces are extruded rigid uPVC.
Door Panel
•	Door Panel consists of extruded rigid uPVC [with optional foam insulation]. 
•	Panel members are mitered and heat-fused to provide a fully welded corner assembly.
•	Vent panel is fully operable for ventilation.
•	Vent panels have two adjustable rollers, set on a stainless steel track cap.  
•	Contains sealed insulating glass.
Weatherstripping
•	Fin-type pile around perimeter of panels.
Glazing System
•	Quality fully-tempered float glass complying with ASTM C 1036.
•	Exterior face-glazed sealed insulating glass. 
•	¾” Dual-Pane insulating glass [[Advanced] [NaturalSun] [SunDefense™] Low-E coated [with Argon]] [[NaturalSun+] [SunDefense+] Low-E with argon]] [[Bronze, Advanced] [Gray] Low-E coated [with Argon]] [Obscure2] [High Altitude1].
-or-
•	1" Dual Pane Low-E insulating glass with Blinds-Between-The-Glass.
-or-
•	1” Triple-Pane insulating glass [Advanced Low-E coated with argon] [NaturalSun Low-E coated with argon] [Obscure2] [High Altitude1].
Interior / Exterior
•	Frame and panel members are [[White] [Almond] [Fossil] with integral color extruded throughout the profiles] [[Brown] [Black] laminate exterior, consisting of a solar reflective coating exceeding AAMA 307 test requirements, with White integral color extruded throughout the profiles on the interior].
•	All exposed PVC surfaces are smooth, glossy and uniform in appearance.
Hardware
•	Interior handle and thumb-lock; finish is [[White] [Almond] [Fossil] to match interior finish] [Satin Nickel] [Oil-Rubbed Bronze].
•	Exterior handle finish Matches exterior finish.
•	Keylock with K-keyway cylinder. Finish is [Chrome].
•	All fasteners are a corrosion-resistant material compatible with uPVC.
•	Multi-point lock, [electroplated steel] [stainless steel].
•	Door rollers are adjustable, permanently sealed, [electroplated steel with organic coated ball-bearing rollers] [corrosion resistant stainless steel, ball bearing rollers].
Screen
•	InView™ Screens
•	Vinyl-coated 18/18 mesh fiberglass screen cloth complying with SMA 1201, set in aluminum extruded frame fitted to door exterior, supplied complete with all necessary hardware.
•	Supplied with four self-adjustable rollers, latch and latch handle.
•	Frame of screen matches exterior frame color.

Optional Products	
Hardware
•	Footbolt, available in colors to match White, Tan or Fossil interior finishes.
Grilles
•	Grilles-Between-the-Glass
•	Insulating glass contains [3/4" contoured] [5/8” Flat (dual-pane glass only)] aluminum grilles permanently installed between two panes of glass (exterior air-space on triple-pane insulating glass).
•	Patterns are [Traditional] [6-Lite Prairie] [9-Lite Prairie] [Top Row] [Custom–Equally Divided].
•	Interior grille color matches interior frame. 
•	Exterior grille color [3/4” Grille is [White] [Almond3] [Brown] [Black] [[5/8” flat Grille is [White] [Almond3] [Brown]].
Blinds
•	Blinds-Between-the-Glass - (select sizes and air-filled glass configurations only)
•	[White] [Slate Gray] [Espresso] aluminum blind sealed between dual-pane Low-E insulating glass.
•	Cordless tilt, raise and lower operation.

(1) Dual-Pane IG High Altitude glazing is available with or without Argon. Triple-Pane IG High Altitude glazing is only available without Argon.
(2) Obscure glass not available with Bronze Advanced, SunDefense+ or NaturalSun+ Low-E IG.
(3) Almond grilles only available on almond units. Almond units with grilles will have an almond grille color.
(4) Available only on doors with White, Almond or Brown exterior finish.