Pella® Vinyl Windows and Doors Complimentary Products 
Pella 250 Series Sliding Patio Door
Detailed Product Description

Standard:
Frame
•	Overall frame depth: 5-15/16".
•	Frame members are mitered and [heat-fused fully welded] [knock-down]. Sill is fitted with weeps.
•	Frame: [1” setback for nail fin for 4-15/16” wall depth and 1-3/8” setback for nail fin for 4-1/2” wall depth] [Block Frame for 5-15/16” wall depth] [Flush Flange for 5-11/16” wall depth].
•	Interior and exterior frame surfaces are extruded rigid uPVC.
Door Panel
•	2-3/4” x 1-3/4" vinyl panel with internal aluminum reinforcement.
•	Door panel consists of extruded, rigid uPVC.
•	Panel members are mitered and heat-fused to provide a fully welded corner assembly.
•	Vent panel is fully operable for ventilation.
•	Vent panels have two adjustable rollers, set on an anodized aluminum track.
•	Contains sealed insulating glass.
Weatherstripping
•	Fin-type pile around perimeter of panels.
Glazing System
•	Interior face-glazed sealed insulating glass. 
•	Standard Dual-Pane tempered glass, with optional Triple-Pane upgrade.
•	7/8” Dual-Pane insulating glass [Advanced Low-E coated [with argon]] [SunDefense™ Low-E coated [with argon]] [High Altitude1].
-or-
•	1-1/4” Triple-Pane insulating glass [SunDefense™ Low-E coated [with argon]] [High Altitude1].
Interior / Exterior
•	Frame and panel members are [[White] [Beige] with integral color extruded throughout the profiles] [[Brown] [Black] laminate exterior, with White integral color extruded throughout the profiles on the interior].
•	Sill: [[Bronze Anodized] [Mill]] finish options.
•	All exposed PVC surfaces are smooth, glossy and uniform in appearance.
Hardware
•	Interior handle and thumb-lock; finish is [[White] [Beige] to match interior finish] [Black].
•	Exterior handle with optional keylock; finish is [[White] [Beige] [Black] to match exterior finish].
•	Optional upgraded hardware; Signature [[White] [Beige] [Black] [Satin Nickel] with optional keylock].
•	Anti-Slam and double-point lock. Meets the most stringent forced entry resistance testing. 
•	Adjustable roller: [Stainless Steel].
Screen
•	Frame of screen is color-matched to exterior frame color.
•	Integrated screen channel in the frame with aluminum screen track for ease of operation and long-term durability.

(1) Dual-Pane IG High Altitude glazing is only available without Argon. Triple-Pane IG High Altitude glazing is only available without Argon.

Premium:
Frame
•	Overall frame depth: 5-15/16".
•	Frame members are mitered and [heat-fused fully welded] [knock-down]. Sill is fitted with weeps.
•	Frame: [1” setback for nail fin for 4-15/16” wall depth and 1-3/8” setback for nail fin for 4-1/2” wall depth] [Block Frame for 5-15/16” wall depth] [Flush Flange for 5-11/16” wall depth].
•	Interior and exterior frame surfaces are extruded rigid uPVC.
Door Panel
•	3-3/4” x 1-3/4" vinyl panel with internal aluminum reinforcement.
•	Door panel consists of extruded, rigid uPVC.
•	Panel members are mitered and heat-fused to provide a fully welded corner assembly.
•	Vent panel is fully operable for ventilation.
•	Vent panels have two adjustable rollers, set on an anodized aluminum track.
•	Contains sealed insulating glass.
Weatherstripping
•	Fin-type pile around perimeter of panels.
Glazing System
•	Interior face-glazed sealed insulating glass. 
•	Standard Dual-Pane tempered glass, with optional Triple-Pane upgrade.
•	7/8” Dual-Pane insulating glass [Advanced Low-E coated [with argon]] [SunDefense™ Low-E coated [with argon]] [High Altitude1].
-or-
•	1-1/4” Triple-Pane insulating glass [SunDefense™ Low-E coated [with argon]] [High Altitude1].
Interior / Exterior
•	Frame and panel members are [[White] [Beige] with integral color extruded throughout the profiles].
•	[Brown] laminate exterior, with White integral color extruded throughout the profiles on the interior.
•	[Black] laminate exterior, with optional [Black] laminate interior or White integral color extruded throughout the profiles on the interior.
•	Sill: [[Bronze Anodized] [Mill]] finish options.
•	All exposed PVC surfaces are smooth, glossy, and uniform in appearance.
Hardware
•	Signature handle; finish is [[White] [Beige] [Black] to match interior and exterior finish]] [Satin Nickel] with optional keylock.
•	Optional upgraded hardware; Flush [[White] [Black] [Satin Nickel]] with optional keylock.
•	Anti-Slam and double-point lock. Meets the most stringent forced entry resistance testing. 
•	Adjustable roller: [Stainless Steel.
Screen
•	Frame of screen is color-matched to exterior frame color.
•	Integrated screen channel in the frame with aluminum screen track for ease of operation and long-term durability.

(1) Dual-Pane IG High Altitude glazing is only available without Argon. Triple-Pane IG High Altitude glazing is only available without Argon.