Pella Corporation		March 2021
102 Main Street
Pella, Iowa 50219
Toll Free	800-54-PELLA
Phone	641-621-1000
Website	www.pella.com
Email	info@pella.com
Guide Specification
Specifier Notes:  This guide specification is written in Construction Specifications Institute (CSI) 3-Part Format in accordance with The CSI Construction Specifications Practice Guide, MasterFormat, SectionFormat, and PageFormat.
This Section must be carefully reviewed and edited by the Architect to meet the requirements of the Project and local building code.  Coordinate this Section with Conditions of the Contract, Division 01, other specification sections, and the Drawings.  Delete all Specifier Notes after editing this Section.
Section numbers and titles are based on CSI MasterFormat 2018 Edition.
SECTION	 08 32 19
SLIDING WOOD-FRAMED GLASS PATIO DOORS
Specifier Notes:  This Section covers Pella Corporation “Pella Reserve” and “Architect Series” multi-slide wood patio doors with aluminum-clad exterior.  Consult Pella Corporation for assistance in editing this Section as required for the Project.
PART 1	GENERAL
1.1	SECTION INCLUDES
A.	Multi-slide wood patio doors with aluminum-clad exterior.
1.2	RELATED REQUIREMENTS
Specifier Notes:  Edit the following list of related sections as required for the Project.  Limit the list to sections with specific information that the reader might expect to find in this Section, but is specified elsewhere.
A.	Section 07 27 00 – Air Barriers:  Water-resistant barriers.
B.	Section 07 92 00 – Joint Sealants:  Sealants.
1.3	REFERENCE STANDARDS
Specifier Notes:  List reference standards used elsewhere in this Section, complete with designations and titles.  Delete reference standards from the following list not used in the edited Section.
A.	American Architectural Manufacturers Association (AAMA):
1.	AAMA 502 – Voluntary Specification for Field Testing of Newly Installed Fenestration Products.
2.	AAMA 2604 – Voluntary Specification, Performance Requirements and Test Procedures for Pigmented Organic Coatings on Aluminum Extrusions and Panels (with Coil Coating Appendix).
3.	AAMA 2605 – Voluntary Specification, Performance Requirements and Test Procedures for Superior Performing Organic Coatings on Aluminum Extrusions and Panels.
B.	ASTM International (ASTM):
1.	ASTM C 1048 – Standard Specification for Heat-Strengthened and Fully Tempered Flat Glass.
2.	ASTM E 330 / E 330M – Standard Test Method for Structural Performance of Exterior Windows, Doors, Skylights and Curtain Walls by Uniform Static Air Pressure Difference.
3.	ASTM F 842 – Standard Test Methods for Measuring the Forced Entry Resistance of Sliding Door Assemblies, Excluding Glazing Impact.
4.	ASTM G 85 – Standard Practice for Modified Salt Spray (Fog) Testing.
C.	Window and Door Manufacturers Association (WDMA):
1.	AAMA/WDMA/CSA 101/I.S.2/A440 – North American Fenestration Standard/Specification for Windows, Doors, and Skylights.
2.	WDMA I.S. 4 – Industry Specification for Preservative Treatment for Millwork.
1.4	PREINSTALLATION MEETINGS
Specifier Notes:  Edit the Preinstallation Meetings article as required for the Project.  Delete this article if not required.
A.	Convene preinstallation meeting [1 week]  [2 weeks] before start of installation of multi-slide patio doors.
B.	Require attendance of parties directly affecting Work of this Section, including Contractor, Architect, installer, and manufacturer’s representative.
C.	Review the Following:
1.	Materials.
2.	Installation.
3.	Field quality control.
4.	Adjusting.
5.	Cleaning.
6.	Protection.
7.	Coordination with other Work.
1.5	SUBMITTALS
Specifier Notes:  Edit the Submittals article as required for the Project.  Delete submittals not required.
A.	Submittals:  Comply with Division 01.
B.	Product Data:  Submit manufacturer’s product data, including installation instructions.
C.	Shop Drawings:  Submit manufacturer’s shop drawings, indicating dimensions, tolerances, materials, components, fabrication, fasteners, weatherstripping, hardware, finish, options, and accessories.
Specifier Notes:  Delete the following sentence if samples are not required.
D.	Samples:  Submit manufacturer’s full-size or partial full-size sample of multi-slide patio doors illustrating glazing system, weatherstripping, quality of construction, and color of finish.
E.	Manufacturer’s Certification:  Submit manufacturer’s certification that materials comply with specified requirements and are suitable for intended application.
F.	Manufacturer’s Project References:  Submit manufacturer’s list of 10 successfully completed multi-slide patio door projects of similar size and scope to this Project, including project name and location, name of architect, and type and quantity of multi-slide patio doors furnished.
G.	Installer’s Project References:  Submit installer’s list of 10 successfully completed patio door projects of similar size and scope to this Project, including project name and location, name of architect, and type and quantity of patio doors installed.
H.	Cleaning and Maintenance Instructions:  Submit manufacturer’s cleaning and maintenance instructions.
I.	Warranty Documentation:  Submit manufacturer’s standard warranty.
1.6	QUALITY ASSURANCE
A.	Manufacturer’s Qualifications:  Manufacturer regularly engaged in the manufacturing of multi-slide patio doors of similar type to that specified for a minimum of 10 years.
B.	Installer's Qualifications:
1.	Installer regularly engaged in installation of patio doors of similar type to that specified for a minimum of 5 years.
2.	Use persons trained for installation of patio doors.
C.	Mock-ups:
1.	Provide sample installation for field testing door performance and to determine acceptability of door installation methods.
2.	Approved mock-ups shall represent minimum quality required for the Work.
Specifier Notes:  Edit the following sentence as required for inclusion of the mock-ups.
3.	Approved mock-ups shall [not] remain in place within the Work.
1.7	DELIVERY, STORAGE, AND HANDLING
A.	Delivery Requirements:
1.	Deliver materials to site undamaged in manufacturer's original, unopened containers and packaging, with labels clearly identifying manufacturer and product name.
2.	Include installation instructions.
B.	Storage and Handling Requirements:
1.	Store and handle materials in accordance with manufacturer's instructions.
2.	Keep materials in manufacturer’s original, unopened containers and packaging until installation.
3.	Store doors off floor or ground.
4.	Provide full support under framework when storing, handling, and installing doors.
5.	Allow sufficient spacing between doors during storage for ventilation.
6.	Do not lift doors by head member only.
7.	Protect doors from weather, direct sunlight, and construction activities.
8.	Protect materials and finish during storage, handling, and installation to prevent damage.
1.8	AMBIENT CONDITIONS
A.	Do not install patio doors under ambient conditions outside manufacturer’s limits.
1.9	WARRANTY
A.	Warranty Period:  10 years with 20-year nonlaminated insulating glass.
PART 2	PRODUCTS
2.1	MANUFACTURERS
A.	Manufacturer:  Pella Corporation, 102 Main Street, Pella, Iowa 50219.  Toll Free 800-54-PELLA.  Phone 641-621-1000.  www.pella.com.  info@pella.com.
Specifier Notes:  Specify if substitutions will be permitted.
B.	Substitutions:  [Not permitted]  [Comply with Division 01].
C.	Single Source:  Provide materials from single manufacturer.
2.2	PERFORMANCE REQUIREMENTS
Specifier Notes:  Performance ratings for “Pella Reserve” and “Architect Series” multi-slide wood patio doors vary by product and size.  Current performance information is found in the Pella Architectural Design Manual at www.pellaadm.com.  Consult Pella for more information.
A.	Performance:
1.	Sliding Door:  Meet or exceed AAMA/WDMA/CSA 101/I.S.2/A440 ratings, [SD-LC25]  [SD-R15], WDMA Hallmark Certified.
2.	Unit Assembly:  Withstand both positive and negative uniform static air pressure difference without damage, ASTM E 330.
3.	Air Infiltration, 1.57 psf wind pressure:  0.15 cfm/ft2 of frame.
4.	Design Pressure:  25 psf.
5.	Water Resistance:  3.76 psf.
B.	Forced Entry Resistance, ASTM F 842, Minimum Security Grade:  10.
C.	Meets U.S. ENERGY STAR guidelines.
2.3	MULTI-SLIDE PATIO DOORS
A.	Multi-Slide Patio Doors:  [Pella Reserve]  [Architect Series] multi-slide wood patio doors with aluminum “EnduraClad” exterior.
B.	Frame:
1.	Select softwood and softwood plywood, immersion treated with “EnduraGuard” wood protection formula in accordance with WDMA I.S. 4 for protection against effects of moisture, decay, stains from mold and mildew, and protection against termite damage.
Specifier Notes:  Specify type of wood for interior exposed surfaces.
2.	Interior Exposed Surfaces:  [Pine]  [Mahogany], edge-banded and veneered.
3.	Exterior Surfaces:  Clad with aluminum at head and jambs.
4.	Head and Jamb Components:  Assembled with screws and staples.
5.	Extruded Aluminum Sill Tracks and Sill Track Covers:  Bonded to stainless steel sill pan with 3M VHB tape.
a.	Stainless Steel Track Caps:  On which the rollers glide.
Specifier Notes:  Specify sill finish.
6.	Sill Finish:  [Painted solar reflective black]  [Painted “clear” morning sky gray].
Specifier Notes:  Refer to overall track depth for frame depth dimension.
7.	Frame Depth:  Varies from 5.92 inches to 22.42 inches, depending on configuration.
Specifier Notes:  Include ONE of the following TWO sentences.
8.	1-1/2-Inch Weep Sill and Surface-Mount Sill Tracks:  Run continuous length of frame width.  Ramps run length of daylight opening only (not in pocket).
9.	Integrated Sill:  [Continuous length of frame]  [Staggered under panel travel] for field-installed finished flooring between sill tracks.
C.	Door Panels:
1.	Material:  Select softwood, immersion treated with “EnduraGuard” wood protection formula in accordance with WDMA I.S. 4 for protection against effects of moisture, decay, stains from mold and mildew, and protection against termite damage.
Specifier Notes:  Specify type of veneer.
2.	Interior Exposed Surfaces:  [Pine]  [Mahogany]  [Douglas fir] veneer.
3.	Exterior Surfaces:  Clad with aluminum.
4.	Panel Stiles:  LVL core with finger-jointed edge bands on both sides and veneered on both faces.
5.	Panel Rails:  Three-ply construction, randomly finger-jointed blocks laminated with water-resistant glue and veneered on both sides.
6.	Corners:  Secured with metal fasteners and structural adhesive.
7.	Panel Thickness:  2-1/16 inches.
Specifier Notes:  Specify panel exterior profile. Contemporary units have Square profiles on the interior and exterior. The Pella Reserve brand has an optional Putty glaze exterior profile.
8.	Panel Exterior Profile:  [Ogee]  [Putty glaze]  [Square].
9.	Panel Interior Profile:  [Ogee]  [Square].
Specifier Notes:  ABEC 5, sealed, electroplated steel, ball-bearing rollers are standard.  Corrosion-resistant, stainless steel, ball-bearing rollers are an out-of-unit option.
Include ONE of the following TWO sentences.
10.	Vent Panels:  Two adjustable, ABEC 5, sealed, electroplated steel, ball-bearing rollers with organic coating, set on stainless steel track.
11.	Vent Panels:  Two adjustable, corrosion-resistant, stainless steel, ball-bearing rollers.
D.	Weatherstripping:
1.	Heads on Interior and Exterior of Panels:  Mohair.
2.	Jambs:  Dual-durometer, extruded-polymer, leaf weatherstrip and mohair rain screen.
3.	Bottom of Panels on Interior and Exterior:  Dual-durometer, extruded-polymer bulb.
4.	Panel Interlockers:  Mohair.
E.	Glazing System:
Specifier Notes:  Custom and high-altitude glazing is available.  Consult Pella for information.
1.	Fully Tempered Float Glass:  ASTM C 1048.
Specifier Notes:  Specify type of glazing required.
Insulating glass with argon is Low-E coated.  All other insulated glass is air filled.
Include ONE of the following TWO paragraphs.
2.	Insulating Glass:  Silicone-glazed, dual-pane, 13/16-inch, dual-seal insulating glass.
a.	[Clear.]
b.	[Obscure.]
c.	[Advanced Low-E with argon.]
d.	[SunDefense Low-E with argon.]
e.	[AdvancedComfort Low-E with argon.]
f.	[NaturalSun Low-E with argon.]
g.	[Bronze Advanced Low-E with argon.]
h.	[Gray Advanced Low-E with argon.]
i.	[Green Advanced Low-E with argon.]
j.	[Reflective bronze.]
3.	Laminated Glass:  Silicone-glazed, dual-pane, 13/16-inch, dual-seal, non-impact laminated glass.
a.	[Clear.]
b.	[Advanced Low-E with argon.]
c.	[SunDefense Low-E with argon.]
d.	[Bronze Advanced Low-E with argon.]
e.	[Gray Advanced Low-E with argon.]
f.	[Green Advanced Low-E with argon.]
F.	Exterior:
Specifier Notes:  AAMA 2603, 2604, and 2605 are the most commonly referenced exterior finish quality standards for painted aluminum.  Pella aluminum-clad products are offered with two quality levels of paint finish, “EnduraClad” and “EnduraClad Plus”.  Pella “EnduraClad” finish meets or exceeds all AAMA 2604 requirements, which possesses the distinguishing characteristic of an elevated resistance to abrasion and corrosion.  Pella “EnduraClad Plus” finish meets or exceeds all AAMA 2605 requirements, which possesses the distinguishing characteristic of an elevated resistance to fade.  This quality makes “EnduraClad Plus” an excellent choice for deeper, more fade-prone color selections in areas of high UV exposure.
Pella “EnduraClad” and “EnduraClad Plus” exterior finish systems are also tested to the following ASTM G 85 test method.  Consult Pella for warranty options for seacoast applications.
Standard and custom colors are available.  Consult Pella for more information.
Specify ONE of the following TWO exterior finish systems.  Specify finish color.
1.	Aluminum-Clad Exteriors:  Finished with “EnduraClad” protective finish, in a multi-step, baked-on finish.
a.	Clean and etch aluminum surface of oxides.
b.	Pre-treat with conversion coating.
c.	Top coat with baked-on polyester enamel.
Specifier Notes:  Consult Pella for standard and custom color options.
d.	Color:  ____________.
e.	Performance Requirements of Exterior Aluminum Finishes:  AAMA 2604 and following performance requirements of AAMA 2605.
1)	Dry Film Hardness:  Eagle Turquoise Pencil, H minimum.
2)	Film Adhesion:  1 mm crosshatch, dry, wet, boiling water.
3)	Impact Resistance:  1/10-inch distortion, no film removal.
4)	Chemical Resistance:  10 percent Muriatic acid, 15 minutes.  Mortar pat test, 24 hours.
5)	Detergent Resistance:  3 percent at 100 degrees F, 72 hours.
6)	Corrosion Resistance:  ASTM G 85, A5, 2,000 hours.  Humidity, 3,000 hours.  Salt spray exceeds 3,000 hours.
2.	Aluminum-Clad Exteriors:  Finished with “EnduraClad Plus” protective finish with 70 percent fluoropolymer resin, in a multi-step, baked-on finish.
a.	Clean and etch aluminum surface of oxides.
b.	Pre-treat with chrome phosphate conversion coating.
c.	Pre-treat with chromic acid sealer/rinse.
d.	Top coat with baked-on 70 percent fluoropolymer-based enamel.
Specifier Notes:  Consult Pella for standard and custom color options.
e.	Color:  ____________.
f.	Performance Requirements of Exterior Aluminum Finishes:  All performance requirements of AAMA 2605.
Specifier Notes:  Specify interior finish.  Consult Pella for color options for the factory-prefinished paint and stain.
G.	Interior:  [Unfinished, ready for site finishing]  [Factory primed with 1 coat acrylic latex]  [Factory-prefinished paint]  [Factory-prefinished stain].
1.	Color:  ____________.
H.	Hardware:
Specifier Notes:  Baldwin hardware is optional.
Specify hardware finish.  Hardware finish varies by style.  Consult Pella for finish options.
Include ONE of the next TWO paragraphs.
1.	Standard flush handle style with “SmartKey Security Re-key” technology, brass.
a.	Hardware Finish:  [Baked Enamel White]  [Basked Enamel Brown]  [Baked Enamel Matte Black]  [Bright Brass PVD]  [Satin Nickel PVD]  [Polished Chrome]  [Oil-Rubbed Bronze (Non-living)].
2.	Baldwin sliding patio door hardware styles with “SmartKey Security Re-key” technology.
a.	Hardware Finish:  [Matte Black]  [Bright Brass]  [Satin Nickel]  [Oil-Rubbed Bronze]  [Antique Brass]  [Distressed Bronze]  [Distressed Nickel]  [Polished Chrome]  [Polished Nickel].
3.	Multiple-Point Lock Hardware:  Electroplated steel with stainless steel strikes.
a.	Located on lead vent panel and fixed panel.
b.	Wood plug on fixed panel hides access to fixed panel locking hardware.
4.	Stacking Door with Dual-Vent Option:  Allows traditional “fixed” panel to vent 1 panel width in opposite direction, with matching hardware set on dual-vent panel.
5.	Biparting Doors:  Active handle set and inactive handle set in middle panels.
Specifier Notes:  Specify hardware handle lock lever location.  40.843 inches is typical.
6.	Hardware Handle Lock Lever Location:  From bottom of panel to center of lock thumb turn is [40.843 inches]  [54.843 inches]  [window application of 10.843 inches.]
Specifier Notes:  The following accessories are optional.  Delete accessories not required.
2.4	ACCESSORIES
A.	Grilles:
Specifier Notes:  Include ONE of the following THREE paragraphs if optional grilles are required.
1.	Integral Light Technology Grilles:
a.	Interior Grilles:
Specifier Notes:  Specify ogee or square profile and material. Pella Contemporary units have a Square profile on the interior and exterior.
1)	[Ogee]  [Square] Profile:  [5/8 inch]  [7/8 inch]  [1-1/4 inches]  [2 inches].
2)	Material:  Solid [pine]  [mahogany]  [Douglas fir].
Specifier Notes:  Specify interior surface finish.  Consult Pella for color options for the factory-prefinished paint and stain on pine.
3)	Interior Surface Finish:  [Unfinished, ready for site finishing]  [Factory primed]  [Pine, factory-prefinished paint]  [Pine, factory-prefinished stain].
b.	Exterior Grilles:
Specifier Notes:  Specify profile.
1)	[Putty]  [Ogee]  [Square] Profile:  [5/8-inch]  [7/8-inch]  [1-1/4-inch]  [2-inch].
2)	Material:  Extruded aluminum.
3)	Finish:  Match door cladding.
Specifier Notes:  Specify pattern.
c.	Pattern:  [Traditional]  [Prairie]  [Top Row]  [Cross].
d.	Insulating Glass:  Non-glare spacer between panes of glass.
e.	Grilles:  Adhered to both sides of insulating glass with VHB acrylic adhesive tape and aligned with non-glare spacer.
2.	Grilles-Between-the-Glass:
Specifier Notes:  Available in clear or Low-E insulating glass only.  Consult Pella for information.
a.	Insulating Glass:  3/4-inch contoured aluminum grilles permanently installed between 2 panes of glass.
Specifier Notes:  Specify pattern.
b.	Pattern:  [Traditional]  [Prairie]  [Top Row]  [Cross].
Specifier Notes:  Specify interior color.  Tan, Brown, and Putty interior grilles-between-the-glass colors are available in single-tone (Tan/Tan, Brown/Brown, and Putty/Putty) (Putty mono).  Other interior colors are also available with Tan or Brown exterior.
c.	Interior Color:  [White]  [Black]  [Tan]  [Brown]  [Putty]  [Morning Sky Gray]  [Ivory]  [Sand Dune]  [Harvest]  [Cordovan]  [Brickstone].
Specifier Notes:  Removable Room Side grilles are not available in Contemporary profiles. Specify exterior color.  Appearance of exterior grille color will vary depending on Low-E coating on glass.  Consult Pella for color options.
d.	Exterior Color:  ____________.
3.	Room Side Removable Grilles:
Specifier Notes:  Specify profile and pattern.
a.	Profile:  [3/4-inch Traditional]  [2-inch Traditional]  [1-1/4-inch Colonial]  [2-inch Colonial].
b.	Pattern:  [Traditional]  [Prairie]  [Cross]  [Top Row].
c.	Removable solid pine wood grilles steel-pinned at joints and fitted to sash with steel clips and tacks.
Specifier Notes:  Specify interior finish.  Consult Pella for color options for the factory-prefinished paint and stain on pine.
d.	Interior Finish:  [Unfinished, ready for site finishing]  [Factory primed]  [Pine, factory-prefinished paint]  [Pine, factory-prefinished stain].
Specifier Notes:  Specify exterior finish.  Appearance of exterior grille color will vary depending on Low-E coating on glass.
e.	Exterior Finish:  [Unfinished, ready for site finishing]  [Factory primed]  [Factory prefinished, finish color matched to exterior cladding].
B.	Security Sensors:  Factory-installed, integrated security sensors available in vent units.
PART 3	EXECUTION
3.1	EXAMINATION
A.	Examine rough openings to receive multi-slide patio doors.
1.	Verify rough openings are plumb, level, square, and of proper dimensions.
2.	Verify a minimum of 1-1/2 inches of solid wood blocking is installed around perimeter of rough openings.
B.	Notify Architect of conditions that would adversely affect installation or subsequent use.
C.	Do not proceed with installation until unsatisfactory conditions are corrected.
3.2	INSTALLATION
A.	Install multi-slide patio doors in accordance with manufacturer's instructions.
B.	Install doors plumb, level, square, and without distortion.
C.	Maintain alignment with adjacent work.
D.	Install doors weathertight.
E.	Install doors to be freely operating.
F.	Verify proper operation of operating hardware.
G.	Seal doors to exterior wall cladding with sealant and related backing materials at perimeter of assembly.
H.	Place interior seal around door perimeter to maintain continuity of building thermal and air barrier using insulating-foam sealant.
I.	Leave doors closed and locked.
Specifier Notes:  Field testing is optional.  Delete if not required.  If Field Quality Control is deleted, delete AAMA 502 from Article 1.3 Reference Standards in this Section.
3.3	FIELD QUALITY CONTROL
A.	Field Testing:  Field test multi-slide patio doors in accordance with AAMA 502.
3.4	ADJUSTING
A.	Adjust multi-slide patio doors for proper operation in accordance with manufacturer’s instructions.
B.	Adjust operating hardware to operate smoothly without binding.
C.	Repair minor damages to finish in accordance with manufacturer’s instructions and as approved by Architect.
D.	Remove and replace with new material, damaged components that cannot be successfully repaired, as determined by Architect.
3.5	CLEANING
A.	Clean multi-slide patio doors in accordance with manufacturer's instructions.
B.	Do not use harsh cleaning materials or methods that could damage finish, glass, or hardware.
C.	Remove labels and visible markings.
D.	Keep door tracks clear of dirt and debris.
E.	Keep weep holes open and clear of obstructions.
3.6	PROTECTION
A.	Protect installed multi-slide patio doors to ensure that, except for normal weathering, doors will be without damage or deterioration at time of Substantial Completion.
END OF SECTION