Pella® Hurricane Shield Series
Hinged Patio Doors
Detailed Product Description

Frame
•	Overall frame depth: 5-1/4".  
•	Frame members are mitered and heat-fused to provide a fully welded corner assembly. Sill covered with clear anodized aluminum and is fitted with weeps.
•	Frame: [Block frame] [Nail fin with 1" set back]. 
•	Interior and exterior frame surfaces are extruded rigid PVC.
Door Panels
•	Door Panel consists of extruded, rigid uPVC.
•	Panel members are mitered and heat-fused to provide a fully welded corner assembly. 
•	Vent panel is fully operable for ventilation. 
•	Contains sealed insulating glass. 
Weatherstripping
•	Foam filled leaf seal around perimeter of frame..
Glazing System
•	Quality fully-tempered float glass complying with ASTM C 1036. 
•	Exterior face-glazed sealed insulating glass. 
•	Dual-Pane insulating glass with argon [Advanced Low-E coated] [Turtle Glass] [SunDefense™ Low-E coated] [Neat, SunDefense], [Obscure, SunDefense] [Obscure] [Bronze] [Gray] [Blue]. 
Interior / Exterior
•	All frame and panel members are White with integral color extruded throughout the profiles, consisting of a solar reflective coating exceeding AAMA 613 test requirements. 
•	All exposed PVC surfaces are smooth, glossy and uniform in appearance.
Hardware
•	Interior handle and thumblock; finish is [White].
•	Exterior handle finish is [White] [Black] [Brushed Chrome].
•	Keylock with K-keyway cylinder. Finish is [Chrome].
•	All fasteners are a corrosion-resistant material compatible with PVC.
•	Multi-point lock, [stainless steel].
•	Commercial Grade Adjustable Hinges are [White] [Silver].
Optional Products	
Grilles
•	Grilles-Between-the-Glass
•	Non-Impact Insulating glass contains [[3/4"] [1"] contoured] [5/8" flat] aluminum grilles permanently installed between two panes of glass.
•	Impact-Resistant Insulating glass contains 5/8" flat aluminum grilles permanently installed between two panes of glass.
•	Patterns are [Traditional] [9-Lite Prairie] [Top Row].
•	Grille color matches frame finish 1..  

1) Only 5/8" flat grilles are available in two-tone finishes. Color options may vary depending on glazing selection,
Contact your local sales representative for current color offering