Pella® Vinyl Windows and Doors 
Pella 250 Series Fixed Frame
Detailed Product Descriptions

Frame
•	Overall frame depth: 3-1/4" on all frame types.
•	Frame members are mitered and heat fused to provide a fully welded corner assembly. Sill is fitted with weeps.
•	Frame: [1-1/8” setback nail fin for 2-1/8” wall depth] [nail fin with flat casing for 2-1/8” wall depth1] [Block frame for 3-1/4” wall depth] [Integral 5/8” flange for 3” wall depth]. 
•	Interior and exterior frame surfaces are extruded rigid uPVC.
Glazing System
•	Quality float glass complying with ASTM C 1036.
•	Exterior face-glazed sealed insulating glass. 
•	Dual-Pane insulating glass [[annealed] [tempered]] [[Advanced] [NaturalSun] [SunDefense™] Low-E coated [with Argon]] [[NaturalSun+] [SunDefense+] Low-E with argon]] [Bronze, Advanced Low-E coated [with Argon]] [Obscure3] [High Altitude2].
-or-
•	1" Triple-Pane [[annealed] [tempered]] [[Advanced] [NaturalSun] Low-E coated [with Argon]] [Obscure3] [High Altitude2].
Interior / Exterior
•	Window frame and sash members are [[White] [Almond] [Fossil] with integral color extruded throughout the profiles] [[Brown] [Black] laminate exterior, consisting of a solar reflective coating exceeding AAMA 307 test requirements, with White integral color extruded throughout the profiles on the interior].
•	All exposed PVC surfaces are smooth, glossy and uniform in appearance.
Optional Products	
•	Grilles-Between-the-Glass
•	[Dual-Pane Insulating glass contains [[3/4"] [1"] contoured] [5/8" flat] aluminum grilles permanently installed between two panes of glass] [Triple-Pane Insulating glass contains 3/4" contoured aluminum grilles permanently installed between three panes of glass].
•	Patterns are [Traditional] [9-Lite Prairie] [6-Lite Prairie] [Top Row].
•	Interior grille color matches interior frame. 
•	Exterior grille color [3/4" Grille is [White] [Almond4] [Fossil4] [Brown] [Black]] [1" Flat Grille is [White] [Almond4] [Fossil4]] [5/8" Flat Grille is [White] [Almond4] [Fossil4]].

(1) Flat casing available only to Northeast region, not all color options available at launch. Contact your local sales representative for current offering.
(2) Dual Pane IG High Altitude glazing is available with or without Argon.  Triple Pane IG High Altitude glazings are only available without Argon.
(3) Obscure glass not available with Bronze Advanced, SunDefense+ or NaturalSun+ Low-E IG.
(4) Almond grilles only available on Almond units. Almond units with grilles will have an Almond grille color, Fossil extruded color units with grilles have a Fossil grille color.